{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Menu","Calculator","Tables","Factsheet","2018Rates"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":6,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Menu","index":0,"n_rows":31,"n_cols":1,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["This is a farm business decision calculator that has 4 worksheets. There are fields that can be completed by the user. It is up to 24 columns wide and 55 rows."]
["Welcome to the Custom Farmwork Rate Calculator Menu Page"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["The Custom Farmwork Rate Calculator is an excel worksheet that allows you to calculate what to charge for custom farmwork."]
["Also included are charts of machinery costs that are required for the calculations and a factsheet containing the 2018 Survey of"]
["Custom Farmwork Rates charged in Ontario and a guide to writing custom farmwork agreements. "]
[]
["The Short-term Equipment Rental Rate Calculator is an excel worksheet that allows you to calculate what to charge for short-term"]
["equipment rentals."]
[]
["Developed by John Molenhuis"]
["Business Analysis and Cost of Production Program Specialist"]
["OMAFRA, Brighton"]
["email: john.molenhuis@ontario.ca"]
["2020-04-15T09:50:08.880"]
[]
[]
["End of worksheet"]

{"sheet":"Calculator","index":1,"n_rows":83,"n_cols":30,"rows_kept":83,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Custom Farmwork Rate Calculator"]
[null,"POWER UNIT (TRACTOR OR SELF-PROPELLED MACHINE)"]
[null,"PTO Horsepower",375,"Self Propelled combines"]
[null,"Life (years)",5,"Purchase Price",478000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D4","v":"Self Propelled combines"},"2WD tractors",null,null,"2WD tractors"]
[null,"Interest rate",0.05,"Hours per year",250,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FWA tractors",null,null,"FWA tractors"]
[null,"Acres/year",2575,"Fuel Cost per litre ",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4WD tractors",null,null,"4WD tractors"]
[null,"Acres/hour (see table 5)",10.3,"Fuel Used -litres/hr  (see Table 5)",{"$f":"C4*0.244","v":91.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Self Propelled combines",null,null,"Self Propelled combines"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Self propelled high clearance sprayer",null,null,"Self propelled high clearance sprayer"]
[null,"Annual depreciation rate (%) from Table 3",{"$f":"IF(D4<>\"\",VLOOKUP(D4,DeprRep,4,FALSE),0)","v":5.6},"Annual repair rate (%) from Table 3",{"$f":"IF(D4<>\"\",VLOOKUP(D4,DeprRep,5,FALSE),0)","v":2.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Self propelled forage harvesters",null,null,"Self propelled forage harvesters"]
[null,"Trade in Value**",{"$f":"IF(C10=0,0,E5-(E5*C10/100*C5))","v":344160},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Depreciation"]
[null,"Annual Fixed Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Trade in value"]
[null,"Capital recovery*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Repairs",{"$f":"VLOOKUP(D4,DeprRep,4)","v":3.3}]
[null,"purchase price – trade-in value",null,{"$f":"E5-C11","v":133840}]
[null,"capital recovery factor","x",{"$f":"(C6*(1+C6)^C5)/((1+C6)^C5-1)","v":0.23097479812826807},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(D4,Tables!B5:F24,5)","v":1}]
[null,null,null,{"$f":"D14*D15","v":30913.6669814874}]
[null,"trade-in value x annual interest rate**","+",{"$f":"C11*C6","v":17208}]
[null,"Total Capital recovery",null,null,{"$f":"D16+D17","v":48121.666981487404}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Headers, grain"]
[null,"Insurance & housing = ",null,"purchase price x 1.0 %",{"$f":"E5*0.01","v":4780},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Headers, corn"]
[null,"Total Fixed Cost",null,null,{"$f":"SUM(E18:E20)","v":52901.666981487404},"(A)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grain carts"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plows, discs"]
[null,"Annual Operating Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vertical tillage"]
[null,"Fuel & lubricants( Table 5)  =   ",null,"(litres/hour x hr/yr x fuel cost/L x 1.15)",{"$f":"E8*E6*E7*1.15","v":26306.249999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cultivators, hoes"]
[null,"Repairs =",null,"Annual repair rate x purchase price",{"$f":"E5*E10/100","v":11950},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Harrows"]
[null,"Total Operating Costs",null,null,{"$f":"SUM(E24:E25)","v":38256.25},"(B)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drills"]
[null,"Total Power Unit Costs",null,null,{"$f":"SUM(E26,E21)","v":91157.916981487404},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Row crop planters"]
[null,"+ IMPLEMENT 1 (TILLAGE IMPLEMENT, PTO MACHINE, OTHER)",null,"Headers, corn",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mower/conditioner"]
[null,"Life (years)",5,"Purchase Price",122000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Balers, round"]
[null,"Interest rate",0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Balers, large square"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Balers, small square"]
[null,"Annual depreciation rate (%) from Table 3",{"$f":"IF(D28<>\"\",VLOOKUP(D28,DeprRep,4,FALSE),0)","v":4.4000000000000004},"Annual repair rate (%) from Table 3",{"$f":"IF(D28<>\"\",VLOOKUP(D28,DeprRep,5,FALSE),0)","v":2.8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Manure spreaders"]
[null,"Trade in Value**",{"$f":"IF(C32=\"\",\"\",E29-(E29*C32/100*C29))","v":95160},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mower/conditioner"]
[null,"+ IMPLEMENT 2 (TILLAGE IMPLEMENT, PTO MACHINE, OTHER)",null,"Headers, grain",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Balers, round"]
[null,"Life (years)",{"$f":"C29","v":5},"Purchase Price",60000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Balers, large square"]
[null,"Interest rate",{"$f":"C30","v":0.05},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Balers, small square"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Manure spreaders"]
[null,"Annual depreciation rate (%) from Table 3",{"$f":"IF(D34<>\"\",VLOOKUP(D34,DeprRep,4,FALSE),0)","v":4.4000000000000004},"Annual repair rate (%) from Table 3",{"$f":"IF(D34<>\"\",VLOOKUP(D34,DeprRep,5,FALSE),0)","v":2.5}]
[null,"Trade in Value**",{"$f":"IF(C38=\"\",\"\",E35-(E35*C38/100*C35))","v":46800}]
[null,"Annual Fixed Cost"]
[null,"Capital recovery*"]
[null,"purchase price – trade-in value",null,{"$f":"(E29-C33)+(E35-C39)","v":40040}]
[null,"capital recovery factor","x",{"$f":"(C30*(1+C30)^C29)/((1+C30)^C29-1)","v":0.23097479812826807}]
[null,null,null,{"$f":"D42*D43","v":9248.2309170558528}]
[null,"trade-in value x annual interest rate**","+",{"$f":"(C33*C30)+(C39*C36)","v":7098}]
[null,"Capital recovery",null,null,{"$f":"D44+D45","v":16346.230917055853}]
[]
[null,"Insurance & housing = ",null,"purchase price x 1%",{"$f":"(E35+E29)*0.01","v":1820}]
[null,"Total Fixed Cost",null,null,{"$f":"SUM(E42:E48)","v":18166.230917055851},"(C)"]
[]
[null,"Annual Operating Cost"]
[null,"Repairs =",null,"Annual repair rate x purchase price",{"$f":"(E29*E32/100)+(E35*E38/100)","v":4916}]
[null,"Total Operating costs",null,null,{"$f":"SUM(E51:E52)","v":4916},"(D)"]
[null,"Total Implement Costs",null,null,{"$f":"SUM(E53,E49)","v":23082.230917055851}]
[null," = Annual Machinery Costs  (A+B+C+D) ",null,null,{"$f":"SUM(E54,E27)","v":114240.14789854325},"(E)"]
[null,"Return to Management",0.15,"Operator Labour (self or hired) per Hour  ",22]
[null,null,null,"Labour Allowance for Machine travel, downtime",0.15]
[null," + Profit Margin (return to management, admin. costs) (suggest 15% of machinery costs ( E x 0.15 )",null,null,{"$f":"E55*C56","v":17136.022184781486},"(F)"]
[null," + Operator Labour (self or hired) --- (suggest 15% over machine hr for travel, downtime)  # of machinery hr x 1.15 x wage/h",null,null,{"$f":"E6*E56*(1+E57)","v":6324.9999999999991},"(G)"]
[null,"=    Total Costs     (E+F+G)",null,null,{"$f":"E55+E58+E59","v":137701.17008332475},"(H)"]
[null," = Custom Rate ",null,"Per Acre",{"$f":"E60/C7","v":53.476182556630967}]
[null,null,null,"Per Hour",{"$f":"E60/E6","v":550.80468033329896}]
[null,"* The capital recovery method estimates the annual depreciation and interest costs. It combines depreciation and"]
[null,"interest costs in one calculation. To calculate the capital recovery costs, the capital recovery factor is multiplied by total"]
[null,"depreciation and adds the result of the trade-in value multiplied by the interest rate. Table 4 provides the capital recovery"]
[null,"factors for selected combinations of years and interest rates."]
[null,"** Trade-in value = purchase price – (purchase price x annual depreciation rate (from Table 3) x number of years owned)."]
[null,"*** Interest: Interest calculation is the average annual interest cost of the investment (yours and/or the lender’s) that is tied"]
[null,"up in the machine."]
[]
[]
[null,"Short Term Equipment Rental Rate Calculator"]
[null," +   Machinery Costs   (from Custom Rate Calculator above)",null,null,{"$f":"E55","v":114240.14789854325},"(E)"]
[null," –   Total Fuel and Lubricant cost (if any)  (see Custom Rate Calculator above)",null,null,{"$f":"E24","v":26306.249999999996},"(J)"]
[null,"Return to management percentage",null,null,0.15]
[null," + Profit Margin (return to management, admin. costs) suggest 15 % of Machinery Costs ( E – J) x 0.15 ",null,null,{"$f":"(E73-E74)*E75","v":13190.084684781486},"(K)"]
[null,"=    Total Costs    (E–J+K)                                                                                                     ",null,null,{"$f":"E73-E74+E76","v":101123.98258332473},"(L)"]
[null," = Rental Rate                                  ",null,"Per Acre",{"$f":"E77/C7","v":39.271449546922227}]
[null,null,null,"Per Hour",{"$f":"E77/E6","v":404.49593033329893}]
[null,"Note:  Rental Rates may have minimum daily or weekly rates"]
[]
[]
[null,"End of worksheet"]

{"sheet":"Tables","index":2,"n_rows":54,"n_cols":28,"rows_kept":54,"cut":false,"hidden":false,"merged":[]}
[null,"Tables 4 and 5 scroll right"]
[]
[null,"Table 3, Annual hours of use, optimal life, depreciation and repair rates",null,null,null,null,null,"Table 4. Capital recovery factors",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TABLE 5. Performance, Horsepower and Fuel Requirements of Selected Farm Equipment"]
[null,"Machine","Annual Use (hours)","Optimal Life (years)","Annual Depreciation Rate (% of purchase price) ","Annual Repair Rate (% of purchase price)",null,null,"Interest rate",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PTO HP(1,2)","Acres/hour(2)","Litres/acre","Litres/hour(3)"]
[null,"2WD tractors",300,20,3.3,2.2000000000000002,null,"Year",0.02,0.03,0.04,0.05,0.06,7.0000000000000007E-2,0.08,0.09,0.1,0.11,0.12,0.13,0.14000000000000001,0.15,null,"4–18-in. furrow plow",75,2.8,6.5,18.3]
[null,"FWA tractors",450,15,4.4000000000000004,2.6,null,1,1.02,1.03,1.04,1.05,1.06,1.07,1.08,1.0900000000000001,1.1000000000000001,1.1100000000000001,1.1200000000000001,1.1299999999999999,1.1399999999999999,1.1499999999999999,null,"6–18-in. furrow plow",140,3,11.4,34.200000000000003]
[null,"4WD tractors",450,15,4.4000000000000004,2.5,null,2,0.51500000000000001,0.52300000000000002,0.53,0.53800000000000003,0.54500000000000004,0.55300000000000005,0.56100000000000005,0.56799999999999995,0.57599999999999996,0.58399999999999996,0.59199999999999997,0.59899999999999998,0.60699999999999998,0.61499999999999999,null,"8–18-in. furrow plow",250,5.6,10.9,61.1]
[null,"Self Propelled combines",250,12,5.6,2.5,null,3,0.34699999999999998,0.35399999999999998,0.36,0.36699999999999999,0.374,0.38100000000000001,0.38800000000000001,0.39500000000000002,0.40200000000000002,0.40899999999999997,0.41599999999999998,0.42399999999999999,0.43099999999999999,0.438,null,"24-ft field cultivator",140,9,3.8,34.200000000000003]
[null,"Headers, grain",250,15,4.4000000000000004,2.5,null,4,0.26300000000000001,0.26900000000000002,0.27500000000000002,0.28199999999999997,0.28899999999999998,0.29499999999999998,0.30199999999999999,0.309,0.315,0.32200000000000001,0.32900000000000001,0.33600000000000002,0.34300000000000003,0.35,null,"31-ft field cultivator",225,20.6,2.7,55]
[null,"Headers, corn",100,15,4.4000000000000004,2.8,null,5,0.21199999999999999,0.218,0.22500000000000001,0.23100000000000001,0.23699999999999999,0.24399999999999999,0.25,0.25700000000000001,0.26400000000000001,0.27100000000000002,0.27700000000000002,0.28399999999999997,0.29099999999999998,0.29799999999999999,null,"44-ft field cultivator",270,29.1,2.2999999999999998,66]
[null,"Grain carts",250,20,3.3,2,null,6,0.17899999999999999,0.185,0.191,0.19700000000000001,0.20300000000000001,0.21,0.216,0.223,0.23,0.23599999999999999,0.24299999999999999,0.25,0.25700000000000001,0.26400000000000001,null,"16-ft chisel plow",155,9,4.2,37.9]
[null,"Plows, discs",100,20,3.3,1.5,null,7,0.155,0.161,0.16700000000000001,0.17299999999999999,0.17899999999999999,0.186,0.192,0.19900000000000001,0.20499999999999999,0.21199999999999999,0.219,0.22600000000000001,0.23300000000000001,0.24,null,"21-ft chisel plow",240,12.6,4.7,58.6]
[null,"Vertical tillage",100,20,3.3,3.5,null,8,0.13700000000000001,0.14199999999999999,0.14899999999999999,0.155,0.161,0.16700000000000001,0.17399999999999999,0.18099999999999999,0.187,0.19400000000000001,0.20100000000000001,0.20799999999999999,0.216,0.223,null,"24-ft tandem disk",150,15.1,2.4,36.700000000000003]
[null,"Cultivators, hoes",200,20,3.3,1.5,null,9,0.123,0.128,0.13400000000000001,0.14099999999999999,0.14699999999999999,0.153,0.16,0.16700000000000001,0.17399999999999999,0.18099999999999999,0.188,0.19500000000000001,0.20200000000000001,0.21,null,"30-ft tandem disk",225,15.3,3.6,55]
[null,"Harrows",200,25,2.7,0.5,null,10,0.111,0.11700000000000001,0.123,0.13,0.13600000000000001,0.14199999999999999,0.14899999999999999,0.156,0.16300000000000001,0.17,0.17699999999999999,0.184,0.192,0.19900000000000001,null,"10-ft offset disk",110,6,4.5,26.9]
[null,"Drills",200,15,4.4000000000000004,3,null,11,0.10199999999999999,0.108,0.114,0.12,0.127,0.13300000000000001,0.14000000000000001,0.14699999999999999,0.154,0.161,0.16800000000000001,0.17599999999999999,0.183,0.191,null,"16-ft offset disk",155,9.6,3.9,37.9]
[null,"Row crop planters",100,10,6.7,4,null,12,9.5000000000000001E-2,0.1,0.107,0.113,0.11899999999999999,0.126,0.13300000000000001,0.14000000000000001,0.14699999999999999,0.154,0.161,0.16900000000000001,0.17699999999999999,0.184,null,"21-ft vertical tillage",190,19.600000000000001,2.4,46.4]
[null,"Self propelled high clearance sprayer",200,8,8.3000000000000007,3.5,null,13,8.7999999999999995E-2,9.4E-2,0.1,0.106,0.113,0.12,0.127,0.13400000000000001,0.14099999999999999,0.14799999999999999,0.156,0.16300000000000001,0.17100000000000001,0.17899999999999999,null,"30-ft vertical tillage",270,27.2,2.4,66]
[null,"Mower/conditioner",150,15,4.4000000000000004,2.2999999999999998,null,14,8.3000000000000004E-2,8.8999999999999996E-2,9.5000000000000001E-2,0.10100000000000001,0.108,0.114,0.121,0.128,0.13600000000000001,0.14299999999999999,0.151,0.159,0.16700000000000001,0.17499999999999999,null,"43-ft vertical tillage",370,39.200000000000003,2.2999999999999998,90.4]
[null,"Balers, round",100,15,4.4000000000000004,1.5,null,15,7.8E-2,8.4000000000000005E-2,0.09,9.6000000000000002E-2,0.10299999999999999,0.11,0.11700000000000001,0.124,0.13100000000000001,0.13900000000000001,0.14699999999999999,0.155,0.16300000000000001,0.17100000000000001,null,"12-row strip tillage",290,17.5,4,70.900000000000006]
[null,"Balers, large square",150,15,4.4000000000000004,1.7,null,16,7.3999999999999996E-2,0.08,8.5999999999999993E-2,9.1999999999999998E-2,9.9000000000000005E-2,0.106,0.113,0.12,0.128,0.13600000000000001,0.14299999999999999,0.151,0.16,0.16800000000000001,null,"6R – 30-in. row crop planter",95,7.6,3.1,23.2]
[null,"Balers, small square",100,20,3.3,1,null,17,7.0000000000000007E-2,7.5999999999999998E-2,8.2000000000000003E-2,8.8999999999999996E-2,9.5000000000000001E-2,0.10199999999999999,0.11,0.11700000000000001,0.125,0.13200000000000001,0.14000000000000001,0.14899999999999999,0.157,0.16500000000000001,null,"12R – 30-in. row crop planter",140,15.3,2.2000000000000002,34.200000000000003]
[null,"Self propelled forage harvesters",400,10,6.7,8,null,18,6.7000000000000004E-2,7.2999999999999995E-2,7.9000000000000001E-2,8.5999999999999993E-2,9.1999999999999998E-2,9.9000000000000005E-2,0.107,0.114,0.122,0.13,0.13800000000000001,0.14599999999999999,0.155,0.16300000000000001,null,"16R – 30-in. row crop planter",155,20.399999999999999,1.9,37.9]
[null,"Manure spreaders",100,10,6.7,4.4000000000000004,null,19,6.4000000000000001E-2,7.0000000000000007E-2,7.5999999999999998E-2,8.3000000000000004E-2,0.09,9.7000000000000003E-2,0.104,0.112,0.12,0.128,0.13600000000000001,0.14399999999999999,0.153,0.161,null,"6R – 30-in. minimum-till planter",75,6.4,2.9,18.3]
[null,"Source: Farm Machinery Custom and Rental Rate Guide, Saskatchewan Ministry of Agriculture, 2018–19.",null,null,null,null,null,20,6.0999999999999999E-2,6.7000000000000004E-2,7.3999999999999996E-2,0.08,8.6999999999999994E-2,9.4E-2,0.10199999999999999,0.11,0.11700000000000001,0.126,0.13400000000000001,0.14199999999999999,0.151,0.16,null,"12R – 30-in. minimum-till planter",155,15.3,2.5,37.9]
[null,null,null,null,null,null,null,"Source: Estimating Farm Machinery Costs, Edwards, William, Iowa State University, 2015.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16R – 30-in. minimum-till planter",225,20.399999999999999,2.7,55]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25-ft grain drill",140,11.7,2.9,34.200000000000003]
[null,null,null,null,null,null,null,"Tractor example using Table 3 and 4:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"35-ft grain drill",225,16.3,3.4,55]
[null,null,null,null,null,null,null,null,"310 Horsepower (HP) Four Wheel Drive (4WD) Tractor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-ft presswheel drill",75,5.0999999999999996,3.6,18.3]
[null,"EXAMPLE ","Accumulated Repair Cost Calculation ",null,null,null,null,"Purchase price",470000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-ft presswheel drill",140,8.5,4,34.200000000000003]
[null,"New 375 HP Combine Cost","$660,000 = $478,000 (combine) + $ 122,000 (corn head) + $60,000 (grain head)",null,null,null,null,"Projected use","450 hr per year for 5 years",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"15-ft no-till drill",140,7,4.9000000000000004,34.200000000000003]
[null,"Estimated annual repair rates","2.5% combine",null,null,null,null,"Depreciaton","Estimated total depreciation over the 5 years:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-ft no-till drill",175,9.3000000000000007,4.5999999999999996,42.8]
[null,null,"2.8% corn head",null,null,null,null,null,"= 4.4% annual depreciation rate (from Table 3, 4WD tractors) x 5 years x $470,000 = $103,400 total depreciation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"90-ft sprayer, pull type",95,49.6,0.5,23.2]
[null,"from Table 3","2.5% grain head",null,null,null,null,"Trade-in value","= $470,000 (purchase price) – $103,400 (total depreciation) = $366,600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"90-ft sprayer, self propelled",85,72.5,0.3,20.8]
[null,"Estimated annual repair costs","Combine: $478,000 x 2.5% for an average of $11,950/year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"9-ft mower conditioner",40,4.4000000000000004,2.2000000000000002,9.8000000000000007]
[null,null,"Corn head: $122,000 x 2.8% for an average of $3,416/year",null,null,null,null,"Capital recovery:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"13-ft rotary mower/conditioner",75,9.6999999999999993,1.9,18.3]
[null,null,"Grain head: $60,000 x 2.5% for an average of 1,500/year",null,null,null,null,null,"= (total depreciation x capital recovery factor)+ (trade-in value x interest rate)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Square baler",40,4.4000000000000004,2.2000000000000002,9.8000000000000007]
[null,null,"Total annual repair costs = $11,950 + $3,416 + $1,500 = $16,866 per year",null,null,null,null,null,"= ($103,400 x 0.218 (from Table 5, 3% interest and 5 years)) + ($366,600 x 3%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,000 lb",60,3,4.9000000000000004,14.7]
[null,"Used Machinery","When calculating the depreciation on used machinery, use the actual price paid ",null,null,null,null,null,"= $22,541 + $10,998",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,500 lb",60,4,3.7,14.7]
[null,null,"for the machine minus its expected trade-in or salvage value, divided by the ",null,null,null,null,null,"= $33,539 per year capital recovery (depreciation and interest costs).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Large size square baler",140,16.3,2.1,34.200000000000003]
[null,null,"expected life of the machine on your farm. Increase repair rates to levels ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,000 lb/wrapper",60,3,4.9000000000000004,14.7]
[null,null,"appropriate for the age or number of hours on the machine. Expect to have ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-row forage harvester",140,1.4,24.4,34.200000000000003]
[null,null,"higher than normal repair expenses in the first year of ownership of a",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Self-propelled forage harvester, 6 row, 15 ft",625,5.0999999999999996,11.2,56.8]
[null,null," used machine as you bring it back into top operating shape",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Large forage blower",60,"—","—",14.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine 6R – 30-in. corn hd",275,5.0999999999999996,13.2,67.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine 12R – 30-in. corn hd",375,10.199999999999999,9,91.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine grain head 25 ft",375,7.4,12.4,91.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine grain head 35 ft",375,10.4,8.8000000000000007,91.6]
[null,"End of worksheet",null,null,null,null,null,"End of worksheet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. Power take off horsepower"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2. Source: Illinois Machinery Cost Estimates for 2019, University of Illinois, Department of Agricultural and Consumer Economics, 2019."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3. Source: Nebraska Tractor Test Laboratory, 2008–2017. Tractor fuel consumption results."]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"End of worksheet"]

{"sheet":"Factsheet","index":3,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Double click to view file as an Adobe pdf document"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["End of worksheet"]

{"sheet":"2018Rates","index":4,"n_rows":296,"n_cols":27,"rows_kept":296,"cut":false,"hidden":false,"merged":[]}
[null,"Survey of Ontario Custom Farmwork Rates"]
[null,"charged in 2018"]
[null,"John Molenhuis, OMAFRA,  Business Analysis and Cost of Production Specialist"]
[null,"Infosheet"]
[null,"Survey Details"]
[null,"Survey results of rates charged in 2018 by 200 Ontario custom farmwork operators are summarized on a provincial basis and also by 6 smaller regional areas. "]
[null,"Where available the provincial average 2015 rates are also listed. The 2015 survey is the previous survey to the 2018 survey. "]
[null,"Average Rates "]
[null,"An average rate is given when there are at least 3 reports. The greater the number of reports, the greater the summary reflects the market rates. "]
[]
[null,"What are percentiles and how can you use them?"]
[]
[null,"Percentiles have been used to help show the range of the rates that were charged. For example, in the Provincial Summary, the 15th percentile"]
[null," for corn combining with grain buggy is $43/acre and the 85th percentile is $54/acre. This means that 15% of those surveyed charged $43/acre or less "]
[null,"and 15% charged more than $54. Seventy percent (85th –15th percentile) of all those reporting charged between $43 and $54/acre. The average rate charged was $48/acre."]
[]
[null,"Survey Areas"]
[]
[null,"Area 1"]
[null,"Chatham-Kent, Elgin, Essex, Lambton, Middlesex"]
[null,"Area 2"]
[null,"Brant, Haldimand, Hamilton, Niagara, Norfolk, Oxford"]
[null,"Area 3"]
[null,"Bruce, Dufferin, Grey, Halton, Huron, Peel, Perth, Simcoe, Waterloo, Wellington "]
[null,"Area 4"]
[null,"Durham, Haliburton, Hastings, Kawartha Lakes, Muskoka, Northumberland, Parry Sound, Peterborough, Prince Edward, York"]
[null,"Area 5"]
[null,"Frontenac, Lanark, Leeds-Grenville, Lennox-Addington, Ottawa, Prescott-Russell, Renfrew, Stormont-Dundas-Glengarry"]
[null,"Area 6"]
[null,"Algoma, Cochrane, Kenora, Manitoulin, Nipissing, Rainy River, Sudbury, Thunder Bay, Timiskaming "]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"$CHANGE","%CHANGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAX",{"$f":"MAX(Z37:Z227)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E38-H38","v":0},{"$f":"(E38-H38)/H38","v":{"$error":"#DIV/0!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E40-H40","v":0},{"$f":"(E40-H40)/H40","v":{"$error":"#DIV/0!"}}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E44-H44","v":0},{"$f":"(E44-H44)/H44","v":{"$error":"#DIV/0!"}}]
[]
[null,"Table 8. Survey of Custom Farmwork Rates charged in 2018",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E46-H46","v":0},{"$f":"(E46-H46)/H46","v":{"$error":"#DIV/0!"}}]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2018,"2018 Percentile",null,2015,"# ",2018,"# ",2018,"# ",2018,null,2018,null,2018,null,2018]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"TILLAGE"]
[null,"Moldboard Plow","ac.",44,32.674783549783548,25,39.099999999999994,28.782051282051277,15,32.06666666666667,4,33,18,31.962962962962965,"—","—",4,37.339285714285715,"—","—"]
[null,null,"hr.",36,133.40277777777777,96.25,172.875,130,13,156.38461538461539,"—","—",15,114.46666666666667,"—","—",4,152.625,"—","—"]
[null,"Chisel Plow/Soil Saver","ac.",55,26.1,20.100000000000001,30,24,18,27.222222222222221,12,24.916666666666668,18,24.083333333333332,"—","—",6,31.333333333333332,"—","—"]
[null,null,"hr.",38,221.39473684210526,150,303.60000000000002,190,11,241.63636363636363,8,212.125,14,222.71428571428572,"—","—",5,188,"—","—"]
[null,"Disc -Primary tillage","ac.",36,21.472222222222221,16,25,19,11,21.40909090909091,"—","—",15,21.833333333333332,3,19.666666666666668,5,20.6,"—","—",null,null,null,null,null,{"$f":"E55-H55","v":36.333333333333343},{"$f":"(E55-H55)/H55","v":0.17057902973395936}]
[null,null,"hr.",24,249.33333333333334,120,300,213,6,294,"—","—",11,247.63636363636363,"—","—",4,225,"—","—"]
[null,"Disc -Secondary tillage","ac.",33,18.466329966329965,14.8,25,17,10,17.75,6,18.25,8,19.375,"—","—",8,18.423611111111111,"—","—",null,null,null,null,null,{"$f":"E57-H57","v":37.195652173913032},{"$f":"(E57-H57)/H57","v":0.17545118949958977}]
[null,null,"hr.",23,249.19565217391303,153,354,212,7,280.57142857142856,4,295.625,5,249.2,"—","—",7,191.28571428571428,"—","—"]
[null,"Offset disc","ac.",13,24.607614607614607,15.466666666666667,30,null,4,23,"—","—",3,20.37037037037037,"—","—",6,27.797979797979803,"—","—",null,null,null,null,null,{"$f":"E59-H59","v":{"$error":"#VALUE!"}},{"$f":"(E59-H59)/H59","v":{"$error":"#VALUE!"}}]
[null,null,"hr.",7,191,"—","—","—","—","—","—","—","—","—","—","—",4,154.5,"—","—"]
[null,"Vertical tillage","ac.",56,21.785714285714285,17.25,25.75,20,17,22,9,19.222222222222221,16,20.6875,6,24.333333333333332,7,24.428571428571427,"—","—",null,null,null,null,null,{"$f":"E61-H61","v":60.477272727272748},{"$f":"(E61-H61)/H61","v":0.21445841392649911}]
[null,null,"hr.",44,342.47727272727275,177.25,500,282,12,419.08333333333331,6,308,12,306.83333333333331,6,313.33333333333331,7,325.71428571428572,"—","—"]
[null,"Zone tillage","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"E63-H63","v":3.1999999999999993},{"$f":"(E63-H63)/H63","v":0.13913043478260867}]
[null,"         with fertilizer","ac.",5,26.2,"—","—",23,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,null,"hr.",3,377.33333333333331,"—","—",426,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Strip tillage","ac.",14,28.321428571428573,21.9,35.049999999999997,"",5,29.9,3,36.333333333333336,6,23,"—","—","—","—","—","—",null,null,null,null,null,{"$f":"E66-H66","v":{"$error":"#VALUE!"}},{"$f":"(E66-H66)/H66","v":{"$error":"#VALUE!"}}]
[null,null,"hr.",6,354,"—","—","","—","—","—","—",4,357.25,"—","—","—","—","—","—"]
[null,"V ripping","ac.",3,30.333333333333332,"—","—","",3,30.333333333333332,"—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"(#REF!-#REF!)/#REF!","v":{"$error":"#REF!"}}]
[null,"Field Cultivate","ac.",91,16.374672946101519,12,20,13.944327101469959,25,16.8,13,16.346153846153847,31,14.642857142857144,6,17.166666666666668,14,19.690476190476193,"—","—"]
[null,null,"hr.",63,337.3174603174603,151.79999999999998,525,241,17,337.05882352941177,8,365.125,21,344.47619047619048,4,251.25,12,340.91666666666669,"—","—",null,null,null,null,null,{"$f":"E70-H70","v":7.9444444444444446},{"$f":"(E70-H70)/H70","v":1.1259842519685039}]
[null,"Harrowing","ac.",4,15,"—","—",7.0555555555555554,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Deep tillage/Subsoiling","ac.",12,32,23,40,29,6,32,"—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,-3.78125,-1.7587209302325581E-2]
[null,null,"hr.",8,211.21875,168.66249999999999,243.95,215,3,252.66666666666666,"—","—","—","—","—","—","—","—","—","—"]
[null,"Soil finisher","ac.",5,15.483333333333331,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,"hr.",5,221,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Packer/Rolling","ac.",46,7.9166666666666661,5,10.25,7.3863636363636367,7,8.6428571428571423,6,7.583333333333333,18,7.3425925925925934,4,10.75,11,7.5454545454545459,"—","—",null,null,null,null,null,42.038461538461547,0.28404365904365908]
[null,null,"hr.",26,190.03846153846155,95,300,148,"—","—",4,160.5,9,204.66666666666666,"—","—",9,186.11111111111111,"—","—"]
[null,"Stalk Chopping","ac.",12,17.083333333333332,11.2,24.099999999999998,14,8,20,"—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,-6.5714285714285836,-3.9349871685201099E-2]
[null,null,"hr.",7,160.42857142857142,"—","—",167,4,203,"—","—","—","—","—","—","—","—","—","—"]
[null,"PLANTING"]
[null,"SOYBEANS"]
[]
[null,"Conventional Row Planter","ac.",43,24.325581395348838,20,29.399999999999991,21,13,22.076923076923077,5,27.4,12,23,5,26,8,27,"—","—"]
[null,null,"hr.",24,394.29166666666669,151.19999999999999,544.25,302,7,446.42857142857144,"—","—",6,429,4,314.5,5,341.2,"—","—"]
[null,"Minimum/No-Till Planter","ac.",56,25.741071428571427,22,30,24.836206896551722,21,23.857142857142858,5,23.4,14,24.107142857142858,4,30,12,30.5,"—","—"]
[null,null,"hr.",34,309.02941176470586,175,475.25,346,15,301.73333333333335,3,218.66666666666666,6,385.66666666666669,"—","—",8,316.375,"—","—"]
[]
[null,"Strip tillage planter","ac.",8,26.125,24,29.9,"—","—","—",3,27,3,24.333333333333332,"—","—","—","—","—","—"]
[null,null,"hr.",4,388.25,"—","—","—","—","—","—","—",3,456.33333333333331,"—","—","—","—","—","—"]
[null,"Conventional Drill","ac.",10,23.6,19.049999999999997,28.599999999999994,20,4,21,"—","—",4,23,"—","—","—","—","—","—"]
[null,null,"hr.",4,337.25,"—","—",183,"—","—","—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"E91-H91","v":1.7368421052631575},{"$f":"(E91-H91)/H91","v":7.2368421052631568E-2}]
[null,"No-Till Drill","ac.",57,25.736842105263158,20.399999999999999,30,24,14,23.5,9,22.777777777777779,14,23.142857142857142,10,28.4,9,32.888888888888886,"—","—"]
[null,null,"hr.",43,285.89534883720933,135.6,500,246,9,309.22222222222223,6,238.66666666666666,10,305.39999999999998,10,194,7,378.5,"—","—",null,null,null,null,null,{"$f":"E93-H93","v":1.125},{"$f":"(E93-H93)/H93","v":4.6875E-2}]
[null,"Air Seeder without fertilizer","ac.",24,25.125,22,27.55,24,5,25.2,"—","—",12,24.416666666666668,3,25.666666666666668,3,27.333333333333332,"—","—"]
[null,null,"hr.",15,484.66666666666669,340.5,537.29999999999995,422,3,319.33333333333331,"—","—",8,476.125,"—","—","—","—","—","—"]
[null,"Air Seeder with fertilizer","ac.",33,26.303030303030305,23.8,30,24.53846153846154,6,25.833333333333332,4,26.75,14,25.071428571428573,"—","—",7,28.714285714285715,"—","—",null,null,null,null,null,{"$f":"E96-H96","v":36.086956521739125},{"$f":"(E96-H96)/H96","v":8.9103596349973155E-2}]
[null,null,"hr.",23,441.08695652173913,291.60000000000002,536.4,405,4,467.25,3,311,10,448.5,"—","—",6,476.33333333333331,"—","—"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"(#REF!-#REF!)/#REF!","v":{"$error":"#REF!"}}]
[null,"Table 8. Survey of Custom Farmwork Rates charged in 2018 (cont'd)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E99-H99","v":0},{"$f":"(E99-H99)/H99","v":{"$error":"#DIV/0!"}}]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2018,"2018 Percentile",null,2015,"# ",2018,"# ",2018,"# ",2018,null,2018,null,2018,null,2018,null,null,null,null,null,{"$f":"E101-H101","v":{"$error":"#VALUE!"}},{"$f":"(E101-H101)/H101","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"PLANTING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E103-H103","v":0},{"$f":"(E103-H103)/H103","v":{"$error":"#DIV/0!"}}]
[null,"CORN"]
[null,"Conventional Row Planter"]
[null,"    Row width 29 in. or less"]
[null,"         with starter fertilizer","ac.",14,25.571428571428573,20.95,30,20.815789473684209,8,24.625,"—","—","—","—","—","—","—","—","—","—"]
[null,null,"hr.",5,323.8,"—","—",270,"—","—","—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"E108-H108","v":1.3333333333333321},{"$f":"(E108-H108)/H108","v":6.0606060606060552E-2}]
[null,"         without starter fertilizer","ac.",3,23.333333333333332,"—","—",22,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"    Row width 30 in. or more"]
[null,"         with starter fertilizer","ac.",68,24.886554621848738,20,30,22,17,24.705882352941178,9,24,22,23.954545454545453,7,27.469387755102041,12,26.166666666666668,"—","—"]
[null,null,"hr.",46,330.76086956521738,194.25,485,314.57894736842104,15,314,6,394.33333333333331,10,318.2,5,370.2,10,310.60000000000002,"—","—",null,null,null,null,null,{"$f":"E112-H112","v":3.1666666666666679},{"$f":"(E112-H112)/H112","v":0.15833333333333338}]
[null,"         without starter fertilizer","ac.",12,23.166666666666668,19.3,27.35,20,"—","—","—","—",6,20.666666666666668,"—","—","—","—","—","—"]
[null,null,"hr.",6,430,"—","—",299,"—","—","—","—",3,310,"—","—","—","—","—","—",null,null,null,null,null,0,{"$error":"#DIV/0!"}]
[null,"Minimum/No-Till"]
[null,"    Row width 29 in. or less",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.8571428571428577,0.11428571428571431]
[null,"         with starter fertilizer","ac.",7,27.857142857142858,"—","—",25,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,null,"hr.",3,409.33333333333331,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"         without starter fertilizer","ac.",4,28.5,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"    Row width 30 in. or more"]
[null,"         with starter fertilizer","ac.",28,28.642857142857142,24,33.9,26.15,8,24.75,"—","—",7,27.571428571428573,4,30,7,33.428571428571431,"—","—",null,null,null,null,null,{"$f":"E121-H121","v":26.29411764705884},{"$f":"(E121-H121)/H121","v":9.6315449256625787E-2}]
[null,null,"hr.",17,299.29411764705884,157.19999999999999,390,273,5,197.6,"—","—",5,393,"—","—",4,336.25,"—","—"]
[null,"         without starter fertilizer","ac.",4,28.125,"—","—",26.416666666666668,"—","—","—","—",3,27.5,"—","—","—","—","—","—",null,null,null,null,null,{"$f":"E123-H123","v":0},{"$f":"(E123-H123)/H123","v":{"$error":"#DIV/0!"}}]
[null,"Strip Tillage Planter"]
[null,"    Row width 29 in. or less",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E125-H125","v":{"$error":"#VALUE!"}},{"$f":"(E125-H125)/H125","v":{"$error":"#VALUE!"}}]
[null,"         with starter fertilizer","ac.",3,27.333333333333332,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"    Row width 30 in. or more"]
[null,"         with starter fertilizer","ac.",6,29.333333333333332,"—","—","—","—","—",3,32,"—","—","—","—","—","—","—","—"]
[null,"CEREALS (OATS, BARLEY, WHEAT)"]
[null,"Conventional Drill"]
[null,"         with starter fertilizer","ac.",12,22.333333333333332,16,30,18.6875,4,20.5,"—","—",5,21,"—","—","—","—","—","—",null,null,null,null,null,{"$f":"E131-H131","v":25.958333333333343},{"$f":"(E131-H131)/H131","v":0.15482107355864819}]
[null,null,"hr.",8,193.625,81.399999999999991,349.70000000000005,167.66666666666666,"—","—","—","—",4,99.5,"—","—","—","—","—","—"]
[null,"         without starter fertilizer","ac.",11,22.363636363636363,18,25.5,18,"—","—","—","—",5,22.4,"—","—",3,24.666666666666668,"—","—",null,null,null,null,null,{"$f":"E133-H133","v":17.833333333333343},{"$f":"(E133-H133)/H133","v":0.1165577342047931}]
[null,null,"hr.",6,170.83333333333334,"—","—",153,"—","—","—","—","—","—","—","—",4,202.5,"—","—"]
[null,"No-Till Drill"]
[null,"         with starter fertilizer","ac.",34,27.088235294117649,22,30.1,24,9,25.888888888888889,5,23.8,10,25.7,5,31.2,4,32,"—","—"]
[null,null,"hr.",20,270.45,153.4,457.49999999999994,247,6,250.66666666666666,3,203,6,336,"—","—",3,266.66666666666669,"—","—",null,null,null,null,null,{"$f":"E137-H137","v":0.40909090909091006},{"$f":"(E137-H137)/H137","v":1.7045454545454586E-2}]
[null,"         without starter fertilizer","ac.",22,24.40909090909091,20,29.549999999999994,24,3,24,3,20.333333333333332,9,22,4,28.25,3,31,"—","—"]
[null,null,"hr.",14,259.03571428571428,167.6,310.99999999999977,268,3,246.33333333333334,"—","—",3,206.66666666666666,3,185.66666666666666,3,314.16666666666669,"—","—"]
[null,"Air Seeder without fertilizer","ac.",15,26.4,24.1,30,23.666666666666668,"—","—","—","—",5,25.6,3,25.666666666666668,3,29.666666666666668,"—","—",null,null,null,null,null,{"$f":"E140-H140","v":-36.375},{"$f":"(E140-H140)/H140","v":-8.3047945205479451E-2}]
[null,null,"hr.",8,401.625,341,497,438,"—","—","—","—",3,446.66666666666669,"—","—","—","—","—","—"]
[null,"Air Seeder with fertilizer","ac.",31,25.580645161290324,23.5,29.5,24.210526315789473,5,24.4,5,25,13,24.384615384615383,"—","—",5,29,"—","—",null,null,null,null,null,{"$f":"E142-H142","v":6.2173913043478137},{"$f":"(E142-H142)/H142","v":1.4629156010230149E-2}]
[null,null,"hr.",23,431.21739130434781,307.5,536.4,425,5,428.6,4,306.25,10,458,"—","—",3,506.66666666666669,"—","—"]
[null,"FORAGES"]
[null,"Drill","ac.",28,25.357142857142858,20,30,23.613636363636363,7,21.285714285714285,4,24.5,5,24,5,29,7,28.285714285714285,"—","—",null,null,null,null,null,{"$f":"E145-H145","v":5.1764705882353041},{"$f":"(E145-H145)/H145","v":2.1841648051625757E-2}]
[null,null,"hr.",17,242.1764705882353,154.80000000000001,273.59999999999997,237,3,214,"—","—",3,202.66666666666666,4,212,5,327,"—","—"]
[null,"Brillion Type","ac.",5,21.4,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Broadcast/ATV Spreading","ac.",12,5.5,4.1500000000000004,6.5249999999999995,4.8571428571428568,7,5,"—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"E148-H148","v":25.642857142857139},{"$f":"(E148-H148)/H148","v":0.27279635258358659}]
[null,null,"hr.",7,119.64285714285714,"—","—",94,3,106.66666666666667,"—","—","—","—","—","—","—","—","—","—"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E150-H150","v":0},{"$f":"(E150-H150)/H150","v":{"$error":"#DIV/0!"}}]
[null,"Table 8. Survey of Custom Farmwork Rates charged in 2018 (cont'd)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E151-H151","v":0},{"$f":"(E151-H151)/H151","v":{"$error":"#DIV/0!"}}]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2018,"2018 Percentile",null,2015,"# ",2018,"# ",2018,"# ",2018,null,2018,null,2018,null,2018,null,null,null,null,null,{"$f":"E153-H153","v":{"$error":"#VALUE!"}},{"$f":"(E153-H153)/H153","v":{"$error":"#VALUE!"}}]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"WEED CONTROL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"E155-H155","v":0},{"$f":"(E155-H155)/H155","v":{"$error":"#DIV/0!"}}]
[null,"HERBICIDE (excluding herbicide cost)"]
[null,"Pull-type Sprayer","ac.",32,10.484375,9,12,9.3903225806451616,13,10.423076923076923,3,11.166666666666666,8,10.1875,"—","—",5,11.2,"—","—"]
[null,null,"hr.",26,350.96153846153845,190,510,358,11,395.45454545454544,"—","—",7,396.42857142857144,"—","—",4,237.5,"—","—",null,null,null,null,null,{"$f":"E158-H158","v":0.30896409196589936},{"$f":"(E158-H158)/H158","v":3.2006850964754897E-2}]
[null," Self Propelled  High Clearance\n Sprayer","ac.",79,9.962025316455696,8.6750000000000007,11.074999999999999,9.6530612244897966,18,9.7222222222222214,14,9.9642857142857135,29,9.9051724137931032,4,10.625,9,10.305555555555555,5,10]
[null,null,"hr.",35,461.53571428571428,300,636.75,511,6,374.16666666666669,5,588,15,483,"—","—",6,438.95833333333331,"—","—",null,null,null,null,null,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"(#REF!-#REF!)/#REF!","v":{"$error":"#REF!"}}]
[null,"MECHANICAL"]
[null,"Inter-row cultivation","ac.",6,18,"—","—",14,"—","—","—","—",3,15.333333333333334,"—","—","—","—","—","—"]
[null,null,"hr.",4,156.25,"—","—",109,"—","—","—","—",3,168.33333333333334,"—","—","—","—","—","—"]
[null,"Rotary Hoe","ac.",6,11.166666666666666,"—","—","",5,11.4,"—","—","—","—","—","—","—","—","—","—"]
[null,"FERTILIZER APPLICATION"]
[null,"Spread dry fertilizer","ac.",40,9.65,8,11,9,10,9.5,7,10.071428571428571,13,9.4230769230769234,4,10.25,5,9.1999999999999993,"—","—"]
[null,null,"hr.",24,376.79166666666669,250,513.75,282,7,379.71428571428572,4,496.25,6,335,"—","—",4,290,"—","—",null,null,null,null,null,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"(#REF!-#REF!)/#REF!","v":{"$error":"#REF!"}}]
[null,"Rental of dry bulk applicator","ac.",3,9.8333333333333339,"—","—",12.4,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,null,"hr.",4,124,"—","—",15.333333333333334,"—","—","—","—",3,15.333333333333334,"—","—","—","—","—","—"]
[null,"Anhydrous","ac.",5,19.8,"—","—",15,4,21.25,"—","—","—","—","—","—","—","—","—","—"]
[null,null,"hr.",3,246.66666666666666,"—","—",212,"—","—","—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"E171-H171","v":3.65034965034965},{"$f":"(E171-H171)/H171","v":0.36224843858431643}]
[null,"Liquid -  ground","ac.",11,13.727272727272727,9.75,16.75,10.076923076923077,4,12.375,5,14.5,"—","—","—","—","—","—","—","—"]
[null,null,"hr.",6,532.5,"—","—",376.33333333333331,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Liquid side -dress","ac.",22,13.659090909090908,10,18,13.227272727272727,12,14.291666666666666,3,13,3,12,"—","—",4,13.5,"—","—",null,null,null,null,null,{"$f":"E174-H174","v":18.133333333333326},{"$f":"(E174-H174)/H174","v":6.9476372924648755E-2}]
[null,null,"hr.",15,279.13333333333333,132.80000000000001,391.5,261,8,255.625,"—","—","—","—","—","—",4,246.75,"—","—"]
[null,"Prescription map service","ac.",4,2.0625,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"(#REF!-#REF!)/#REF!","v":{"$error":"#REF!"}}]
[null,"Site specific soil sampling","ac.",4,11.625,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"INSECTICIDE/FUNGICIDE"]
[null,"Early season application","ac.",7,10.464285714285714,"—","—",10,"—","—","—","—",5,10,"—","—","—","—","—","—"]
[null,null,"hr.",5,358.75,"—","—",426,"—","—","—","—",3,366.66666666666669,"—","—","—","—","—","—"]
[null,"Late season application","ac.",11,11.204545454545455,10,14,11,"—","—",3,13.333333333333334,6,10,"—","—","—","—","—","—"]
[null,null,"hr.",8,497.96875,302.5,742.5,"","—","—","—","—",4,462.5,"—","—","—","—","—","—"]
[]
[null,"Survey of Custom Farmwork Rates charged in 2018"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2018,"2018 Percentile",null,2015,"# ",2018,"# ",2018,"# ",2018,null,2018,null,2018,null,2018]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"COMBINING "]
[null,"CORN"]
[null,"         with grain buggy","ac.",113,47.929203539823007,43,54,44,32,45.21875,15,50,35,47.114285714285714,11,49.090909090909093,19,51.578947368421055,"—","—"]
[null,null,"hr.",73,381.55479452054794,236.99999999999997,500,375,22,369.63636363636363,9,354.27777777777777,24,427.375,6,323.5,11,362.27272727272725,"—","—"]
[null,"         without grain buggy","ac.",21,43.047619047619051,40,46,44,4,40.25,"—","—",9,44.666666666666664,"—","—",6,43.5,"—","—"]
[null,null,"hr.",9,323.66666666666669,178.4,452,182,"—","—","—","—",3,240.33333333333334,"—","—",3,349.33333333333331,"—","—"]
[null,"SOYBEANS"]
[null,"         with grain buggy","ac.",118,46.290960451977398,42,50.45,43.459595959595958,33,43.621212121212125,17,47.529411764705884,36,45.305555555555557,11,48.18181818181818,19,51.473684210526315,"—","—"]
[null,null,"hr.",70,518.65714285714284,350,750,504,22,521.86363636363637,10,563.29999999999995,23,565.95652173913038,5,330.4,8,486,"—","—"]
[null,"         without grain buggy","ac.",24,42.947916666666664,40.450000000000003,46,42,5,40,"—","—",10,44.475000000000001,"—","—",6,43.5,"—","—"]
[null,null,"hr.",9,430.44444444444446,259.60000000000002,705.59999999999991,217.33333333333334,"—","—","—","—",3,292.33333333333331,"—","—","—","—","—","—"]
[null,"CEREALS"]
[null,"         with grain buggy","ac.",98,45.38095238095238,40,50,42.380208333333336,21,43.523809523809526,17,46.117647058823529,34,44.514705882352942,10,47.5,13,50.384615384615387,3,35.277777777777779,null,null,null,null,null,{"$f":"E200-H200","v":-36.816666666666663},{"$f":"(E200-H200)/H200","v":-8.199703043801039E-2}]
[null,null,"hr.",60,412.18333333333334,215.1,632.25,449,15,420.86666666666667,10,469.6,22,449.95454545454544,4,264,7,317.42857142857144,"—","—"]
[null,"         without grain buggy","ac.",21,41.791666666666664,40,45,40,3,43.333333333333336,"—","—",10,43.3,"—","—",5,43,"—","—"]
[null,null,"hr.",10,360.9,185.99999999999997,585.89999999999986,120.33333333333333,"—","—","—","—",4,240.25,"—","—","—","—","—","—",null,null,null,null,null,{"$f":"E203-H203","v":0},{"$f":"(E203-H203)/H203","v":{"$error":"#DIV/0!"}}]
[null,"CANOLA"]
[null,"         with grain buggy","ac.",6,41.75,"—","—",44.81818181818182,"—","—","—","—",3,49.333333333333336,"—","—","—","—","—","—",null,null,null,null,null,{"$f":"E205-H205","v":17.083333333333314},{"$f":"(E205-H205)/H205","v":3.6956913647016365E-2}]
[null,null,"hr.",3,479.33333333333331,"—","—",462.25,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"GRAIN BUGGY ALONE","ac.",11,6.5454545454545459,4.5,9,5.1333333333333337,4,5.75,"—","—",3,7.666666666666667,3,5.333333333333333,"—","—","—","—"]
[null,null,"hr.",10,125,82,150,143,"—","—","—","—",3,160,"—","—",3,116.66666666666667,"—","—",null,null,null,null,null,{"$f":"#REF!-#REF!","v":{"$error":"#REF!"}},{"$f":"(#REF!-#REF!)/#REF!","v":{"$error":"#REF!"}}]
[]
[null,"Table 8. Survey of Custom Farmwork Rates charged in 2018 (cont'd)"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2018,"2018 Percentile",null,2015,"# ",2018,"# ",2018,"# ",2018,null,2018,null,2018,null,2018]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"OTHER CROP HARVESTING"]
[null,"Grain swathing","ac.",11,17.106060606060606,14.583333333333332,21,16,"—","—","—","—",4,15.5,"—","—","—","—",3,14.388888888888888]
[null,null,"hr.",11,153.45454545454547,80,188,82.5,"—","—","—","—",4,76.25,"—","—","—","—","—","—"]
[null,"HIGH MOISTURE CORN"]
[null,"    Combined and hauled to Silo","ac.",4,55,"—","—",48.2,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"EDIBLE BEANS"]
[null," Bean Pulling + windrowing","ac.",5,41,"—","—",35,"—","—","—","—",3,45,"—","—","—","—","—","—"]
[null,null,"hr.",4,452.5,"—","—",392,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Combining -Conventional Grain type","ac.",17,50,42,55,44.3,4,48.75,3,55,7,49.857142857142854,"—","—","—","—","—","—",null,null,null,null,null,{"$f":"E222-H222","v":13.166666666666686},{"$f":"(E222-H222)/H222","v":2.9357116313638094E-2}]
[null,null,"hr.",9,461.66666666666669,264,670,448.5,"—","—","—","—",3,430,"—","—","—","—","—","—"]
[null,"Combining -Specialty -Bob/Lilliston ","ac.",9,61.555555555555557,48.4,75,51.25,4,66.25,"—","—",3,56,"—","—","—","—","—","—",null,null,null,null,null,{"$f":"E224-H224","v":{"$error":"#VALUE!"}},{"$f":"(E224-H224)/H224","v":{"$error":"#VALUE!"}}]
[null,null,"hr.",6,525.83333333333337,"—","—","","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"TRUCKING"]
[null,"Grains and Oilseeds","bu.",4,0.17749999999999999,"—","—",0.16,4,0.17749999999999999,"—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"E227-H227","v":-1.8135257827958995E-2},{"$f":"(E227-H227)/H227","v":-2.0330441443304199E-3}]
[null,null,"mt.",71,8.9021126760563369,6.5500000000000007,11.5,8.9202479338842959,15,7.2099999999999991,13,8.4384615384615387,27,8.4203703703703709,10,12.41,6,10.458333333333334,"—","—"]
[null,"FORAGE HARVESTING"]
[null,"HAY"]
[null,"Swathing/Conditioning","ac.",41,18.487611304684474,15,22,17.722222222222221,6,20.666666666666668,3,19.166666666666668,16,17.905753968253968,8,20.875,6,14.666666666666666,"—","—"]
[null,null,"hr.",31,186.43548387096774,111,300,154,4,243.75,"—","—",12,174.25,6,188,5,176.4,"—","—"]
[null,"Raking","ac.",29,11.114942528735634,6.2,15,9,4,15.75,3,12.333333333333334,14,9.5238095238095237,5,12,3,9.6666666666666661,"—","—",null,null,null,null,null,{"$f":"E233-H233","v":55.154166666666683},{"$f":"(E233-H233)/H233","v":0.50417063416492114}]
[null,null,"hr.",20,164.55,80,248.99999999999991,109.39583333333333,"—","—","—","—",8,162.5,5,133.80000000000001,3,143.33333333333334,"—","—"]
[null,"Tedding","ac.",16,12.75,10,15.75,10,4,12.5,"—","—",5,12.2,3,16,"—","—","—","—",null,null,null,null,null,{"$f":"E235-H235","v":67.833333333333343},{"$f":"(E235-H235)/H235","v":0.63395638629283502}]
[null,null,"hr.",12,174.83333333333334,69.5,308.39999999999998,107,"—","—","—","—",3,189.33333333333334,4,232.25,"—","—","—","—"]
[null,"Windrow merging","ac.",10,14.95,11.675000000000001,18.949999999999996,null,"—","—","—","—",3,15.666666666666666,"—","—",3,17.333333333333332,"—","—"]
[null,null,"hr.",9,236.11111111111111,116,384,null,"—","—","—","—",4,252.5,"—","—",3,273.33333333333331,"—","—"]
[null,"Bale - sm. square (ground)","bale",3,1.1166666666666667,"—","—",0.91,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Bale - sm. square (loaded)","bale",15,1.0499999999999998,0.59000000000000008,1.385,0.79705882352941182,3,1.0833333333333333,"—","—",6,0.78333333333333333,3,1.3666666666666665,"—","—","—","—",null,null,null,null,null,{"$f":"E240-H240","v":0.17058375104427714},{"$f":"(E240-H240)/H240","v":0.13477482799503954}]
[null,"Bale - lg. Square  ","ft.",19,1.4362781954887216,1.1499999999999999,1.7249999999999999,1.2656944444444445,"—","—",3,1.5166666666666668,9,1.5071428571428571,"—","—",4,1.35,"—","—"]
[null,"Bale - lg. Round under 1000 lbs.","bale",32,8.671875,7,10,8.01,5,9.3000000000000007,4,10.5,10,7.95,6,8.8333333333333339,7,8.0714285714285712,"—","—"]
[null,"Bale - lg. Round over 1000 lbs.","bale",15,9.5666666666666664,8,12,7.5,"—","—","—","—","—","—",5,11.9,3,8.3333333333333339,"—","—"]
[null,"Entire operation (mowing to baling)  lg. bale",null,5,15.8,"—","—",14.166666666666666,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Baling corn stalks","bale",6,12.333333333333334,"—","—",null,3,12.833333333333334,"—","—","—","—","—","—","—","—","—","—",null,null,null,null,null,{"$f":"E245-H245","v":0},{"$f":"(E245-H245)/H245","v":{"$error":"#DIV/0!"}}]
[null,"BALE WRAPPING"]
[null,"Individual -with plastic","bale",4,10.5,"—","—",9,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Tube","bale",11,6.2727272727272725,4,9.25,4.8149999999999995,"—","—","—","—","—","—",3,7.166666666666667,3,7,"—","—"]
[null,"Hauling hay bales","bale",3,6.333333333333333,"—","—",null,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"STRAW  ",null,null,null,"—","—",null,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Bale - lg. Round ","bale",6,8.5416666666666661,"—","—",7.5625,"—","—","—","—",3,8.0833333333333339,"—","—","—","—","—","—"]
[null,"Table 8. Survey of Custom Farmwork Rates charged in 2018 (cont'd)"]
[]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2018,"2018 Percentile",null,2015,"# ",2018,"# ",2018,"# ",2018,null,2018,null,2018,null,2018]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"HAYLAGE"]
[null,"PT0 Harvester-"]
[null,"      Field Chopping only -","hr.",3,168.33333333333334,"—","—",163,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Self Prop Harvester"]
[null,"      Field Chopping only -","ac.",3,46.592592592592588,"—","—","","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,null,"hr.",7,456.42857142857144,"—","—",395.35714285714283,"—","—","—","—","—","—","—","—",3,391.66666666666669,"—","—"]
[null,"      Chop, Haul, Pack, Blow","hr.",6,770,"—","—",639,"—","—","—","—","—","—","—","—",3,555,"—","—"]
[null,"CORN SILAGE"]
[null,"PT0 Harvester-"]
[null,"      Field Chopping only -","ac.",3,104.33333333333333,"—","—","","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,null,"hr.",3,148.33333333333334,"—","—",198.42857142857142,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Self Prop Harvester"]
[null,"      Field Chopping only -","hr.",3,576.66666666666663,"—","—",null,"—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Self Prop Harvester with kernel processor "]
[null,"      Field Chopping only -","hr.",7,505.71428571428572,"—","—",433,"—","—","—","—",3,508.33333333333331,"—","—",3,533.33333333333337,"—","—"]
[null,"      Chop, Haul, Pack, Blow","hr.",6,656.66666666666663,"—","—",696,"—","—","—","—",3,650,"—","—","—","—","—","—"]
[null,"MANURE HANDLING"]
[null,"SOLID "]
[null,"Loader only","hr.",13,95,79,112.99999999999999,74,4,88.75,"—","—","—","—",4,110,"—","—","—","—"]
[null,"Spreader only","hr.",11,115.90909090909091,82.5,152.5,111,3,115,"—","—","—","—",3,123.33333333333333,"—","—","—","—"]
[null,"Loader and Spreader","hr.",8,152.5,101,200,136,"—","—","—","—",3,96.666666666666671,"—","—","—","—","—","—"]
[null,"LIQUID     "]
[null,"Drag hose boom applicator per 1000 gal",null,8,11.375,10,12.5,10.75,3,11.166666666666666,"—","—",3,12.5,"—","—","—","—","—","—"]
[null,"Drag hose injection             per 1000 gal",null,3,13.5,"—","—","","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Tanker - surface applied only per 1000 gal",null,5,13.8,"—","—",9,"—","—","—","—",4,14.75,"—","—","—","—","—","—"]
[null,"Tanker - surface applied only per hour",null,10,222,133.75,257.49999999999994,165,"—","—","—","—",3,150,3,356.66666666666669,3,141.66666666666666,"—","—"]
[null,"MISCELLANEOUS"]
[null,"Snow Removal - blade","hr.",19,95.526315789473685,75,121.49999999999999,93,5,82,"—","—",6,121.66666666666667,3,101.66666666666667,"—","—","—","—"]
[null,"Snow blowing","hr.",33,120,80,161,100,7,130.71428571428572,3,98.333333333333329,16,127.5,3,143.33333333333334,3,66.666666666666671,"—","—"]
[null,"Table 9.Survey of Short-term Rental Rates charged in 2018"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2018,"2018 Percentile",null,2015,"# ",2018,"# ",2018,"# ",2018,null,2018,null,2018,null,2018]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"TRACTOR RENTALS"]
[null,"Custom Operator","hr.",11,56.272727272727273,27.5,87.5,46,3,68.333333333333329,"—","—",6,39,"—","—","—","—","—","—"]
[null,null,"hp.hr",3,0.31,"—","—",0.49,"—","—","—","—","—","—","—","—","—","—","—","—"]
[]
[]
[]
[]
[null,"End of worksheet"]