{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Menu","Calculator","Tables","Factsheet","2024Rates"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":6,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Menu","index":0,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["This is a farm business decision calculator that has 5 worksheets. There are fields that can be completed by the user. It is up to 28 columns wide and 73 rows."]
["Welcome to the Custom Farmwork Rate Calculator Menu Page"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["The Custom Farmwork Rate Calculator is an excel worksheet that allows you to calculate what to charge for custom farmwork."]
["Also included are charts of machinery costs that are required for the calculations and a factsheet containing the 2024 Survey of"]
["Custom Farmwork Rates charged in Ontario and a guide to writing custom farmwork agreements. "]
[]
["The Short-term Equipment Rental Rate Calculator is an excel worksheet that allows you to calculate what to charge for short-term"]
["equipment rentals."]
["Several of the cells have a red triangle in the upper right hand corner of the cell. By moving your mouse cursor over this triangle, a brief description of the input will be displayed."]
[]
["Developed by John Molenhuis"]
["Business Analysis and Cost of Production Program Specialist"]
["OMAFA, Brighton"]
["email: john.molenhuis@ontario.ca"]
["2025-06-01"]
[]
[]
["End of worksheet"]

{"sheet":"Calculator","index":1,"n_rows":109,"n_cols":44,"rows_kept":109,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Custom Farmwork Rate Calculator"]
[null,"Numbers/text in blue, yellow shaded areas can be edited/changed"]
[null,"GENERAL PARAMETERS"]
[null,"Annual interest rate ***",0.05,"Fuel cost per litre",1.35]
[null,"Insurance and housing rate (% of purchase price)",0.01,"Fuel consumption - litres/engine hp.hr",0.192,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2WD tractor","2WD tractors",null,null,"2WD tractors"]
[null,null,null,"Operator labour (self or hired) rate per hour",27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Front wheel assist tractor","FWA tractors",null,null,"FWA tractors"]
[null,null,null,"Return to management, administration costs",0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4WD tractor","4WD tractors",null,null,"4WD tractors"]
[null,"POWER UNIT (TRACTOR OR SELF-PROPELLED (SP) MACHINE)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tracked tractor","Self Propelled combines",null,null,"Self Propelled combines"]
[null,"Rated engine horsepower",375,"SP Rotary combine",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Rotary combine","Self propelled high clearance sprayer",null,null,"Self propelled high clearance sprayer"]
[null,"Life (years)",{"$f":"IF(D10<>\"\",VLOOKUP(D10,DeprRep,3,FALSE),0)","v":12},"Purchase price",740000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Swather","Self propelled forage harvesters",null,null,"Self propelled forage harvesters"]
[null,"Acres/year",{"$f":"C15*E12","v":2550},"Hours per year",{"$f":"IF(D10<>\"\",VLOOKUP(D10,DeprRep,2,FALSE),0)","v":250},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Forage harvester","Depreciation"]
[null,null,null,"Fuel Used - litres/hour  (see Table 5)",{"$f":"C10*E6","v":72},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Forage harvester header","Trade in value"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Mower/conditioner","Repairs",{"$f":"VLOOKUP(D10,DeprRep,4)","v":3.3000000000000003}]
[null,"Work rate: Acres/hour (see table 5)",{"$f":"C16*C17*(C18*100)/825","v":10.199999999999999},"Annual depreciation rate (%) from Table 3",{"$f":"IF(D10<>\"\",VLOOKUP(D10,DeprRep,4,FALSE),0)","v":5.6000000000000005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP small square bale mover"]
[null,"Average speed (miles per hour)",3.3,"Annual repair rate (%) from Table 3",{"$f":"IF(D10<>\"\",VLOOKUP(D10,DeprRep,5,FALSE),0)","v":2.63},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High clearance sprayers",null,{"$f":"VLOOKUP(D10,Tables!#REF!,5)","v":{"$error":"#REF!"}}]
[null,"Implement width (feet)",30]
[null,"Field efficiency (%)",0.85,"Trade in Value**",{"$f":"IF(E15=0,0,E11-(E11*E15/100*C11))","v":242719.99999999988}]
[]
[null,"Annual Fixed Cost",null,null,"Total annual $","$ per hour","$ per acre",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4–18-in. furrow plow","Rigid headers"]
[null,"Capital recovery*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6–18-in. furrow plow","Pickup headers"]
[null,"purchase price – trade-in value",null,{"$f":"E11-E18","v":497280.00000000012},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8–18-in. furrow plow","Flex headers"]
[null,"capital recovery factor (from Table 4)","x",{"$f":"IFERROR((C5*(1+C5)^C11)/((1+C5)^C11-1),0)","v":0.11282541002081541},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24-ft field cultivator","Draper headers"]
[null,null,null,{"$f":"D22*D23","v":56105.8198951511},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"31-ft field cultivator","Corn headers"]
[null,"trade-in value x annual interest rate**","+",{"$f":"E18*C5","v":12135.999999999995},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"44-ft field cultivator","SP Swather"]
[null,"Total capital recovery",null,null,{"$f":"D24+D25","v":68241.8198951511},{"$f":"IFERROR(E26/$E$12,0)","v":272.96727958060438},{"$f":"IFERROR(F26/$C$15,0)","v":26.76149799809847},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16-ft chisel plow","Grain carts"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"21-ft chisel plow","Powered augers"]
[null,"Insurance & housing = ",null,{"$f":"\"purchase price x \"&$C$6*100&\" %\"","v":"purchase price x 1 %"},{"$f":"E11*C6","v":7400},{"$f":"IFERROR(E28/$E$12,0)","v":29.6},{"$f":"IFERROR(F28/$C$15,0)","v":2.9019607843137258},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24-ft tandem disk","PTO augers"]
[null,"Total Fixed Cost",null,null,{"$f":"SUM(E26:E28)","v":75641.8198951511},302.56727958060441,29.663458782412199,"(A)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30-ft tandem disk","Grain vac"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10-ft offset disk","PT Mower/conditioner (sickle)"]
[null,"Annual Operating Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16-ft offset disk","PT Mower/conditioner (disc)"]
[null,"Fuel (Table 5)  =   ",null,"(litres/hour x hours/year x fuel cost/litre)",{"$f":"E13*E12*E5","v":24300},{"$f":"IFERROR(E32/$E$12,0)","v":97.2},{"$f":"IFERROR(F32/$C$15,0)","v":9.529411764705884},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"21-ft vertical tillage","Hay rake (wheel)"]
[null,"Repairs and maintenance =",null,"annual repair rate x purchase price",{"$f":"E11*E16/100","v":19462},77.847999999999999,7.6321568627450986,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30-ft vertical tillage","Round baler"]
[null,"Total Operating Costs",null,null,{"$f":"SUM(E32:E33)","v":43762},175.048,17.161568627450983,"(B)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"43-ft vertical tillage","Large square baler"]
[null,"Total Power Unit Costs",null,null,{"$f":"SUM(E34,E29)","v":119403.8198951511},477.61527958060441,46.825027409863182,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-row strip tillage","Small square baler"]
[null,"+ IMPLEMENT 1 (TILLAGE IMPLEMENT, PTO MACHINE, OTHER)",null,"Corn headers",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6R – 30-in. row crop planter","PT round bale mover"]
[null,null,null,"12R – 30-in. corn hd",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12R – 30-in. row crop planter","PT large square bale mover"]
[null,"Life (years)",{"$f":"IF(D36<>\"\",VLOOKUP(D36,DeprRep,3,FALSE),0)","v":15},"Purchase Price",170000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16R – 30-in. row crop planter","Air drills (independent openers)"]
[null,"Acres/year",{"$f":"E39*C15","v":1019.9999999999999},"Hours per year",{"$f":"IF(D36<>\"\",VLOOKUP(D36,DeprRep,2,FALSE),0)","v":100},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6R – 30-in. minimum-till planter","Air hoe drills"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12R – 30-in. minimum-till planter","Air disk drills"]
[null,"Trade in Value**",{"$f":"IF(E41=\"\",\"\",E38-(E38*E41/100*C38))","v":57799.999999999985},"Annual depreciation rate (%) from Table 3",{"$f":"IF(D36<>\"\",VLOOKUP(D36,DeprRep,4,FALSE),0)","v":4.4000000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16R – 30-in. minimum-till planter","Air seeder"]
[null,null,null,"Annual repair rate (%) from Table 3",{"$f":"IF(D36<>\"\",VLOOKUP(D36,DeprRep,5,FALSE),0)","v":2.94},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25-ft grain drill","Row crop planters"]
[null,"Annual Fixed Cost",null,null,"Total annual $","$ per hour","$ per acre",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"35-ft grain drill","Plows"]
[null,"Capital recovery*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-ft presswheel drill","Disks"]
[null,"purchase price – trade-in value",null,{"$f":"E38-C41","v":112200.00000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-ft presswheel drill","Cultivators"]
[null,"capital recovery factor (from Table 4)","x",{"$f":"IFERROR((C5*(1+C5)^C38)/((1+C5)^C38-1),0)","v":9.6342287609244348E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"15-ft no-till drill","Standard harrows"]
[null,null,null,{"$f":"D45*D46","v":10809.604669757216},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-ft no-till drill","Heavy harrows"]
[null,"trade-in value x annual interest rate**","+",{"$f":"(C41*C5)","v":2889.9999999999995},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"90-ft sprayer, pull type","Harrow packers",null,null,null,null,null,null,null,null,null,"per hour","implement1","implement2",null,"power + return+operator"]
[null,"Total capital recovery",null,null,{"$f":"D47+D48","v":13699.604669757216},{"$f":"IFERROR(E49/$E$39,0)","v":136.99604669757215},{"$f":"IFERROR(F49/($C$15),0)","v":13.430984970350211},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"90-ft sprayer, self propelled","Vertical tillage tools",null,null,null,null,null,null,null,null,null,"trade in",{"$f":"E38-C41","v":112200.00000000001},{"$f":"E60-C63","v":0},{"$f":"SUM(AN49:AO49)","v":112200.00000000001}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"9-ft mower conditioner","Land roller",null,null,null,null,null,null,null,null,null,"cap recovery rate",{"$f":"D68","v":0}]
[null,"Insurance & housing = ",null,{"$f":"\"purchase price x \"&$C$6*100&\" %\"","v":"purchase price x 1 %"},{"$f":"E38*C6","v":1700},{"$f":"IFERROR(E51/$E$39,0)","v":17},{"$f":"IFERROR(F51/($C$15),0)","v":1.6666666666666667},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"13-ft rotary mower/conditioner","Land scraper",null,null,null,null,null,null,null,null,null,null,{"$f":"AN49*AN50","v":0},{"$f":"AO49*AN50","v":0},{"$f":"SUM(AN51:AO51)","v":0}]
[null,"Total Fixed Cost",null,null,{"$f":"SUM(E45:E51)","v":15399.604669757216},153.99604669757215,{"$f":"IFERROR(F52/($C$15),0)","v":15.097651637016879},"(C)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Square baler","Post pounder",null,null,null,null,null,null,null,null,null,"interest",{"$f":"C41*C39","v":58955999.999999978},{"$f":"C63*C61","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,000 lb","Vertical feed mixer",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AN51:AN52)","v":58955999.999999978},{"$f":"SUM(AO51:AO52)","v":0},{"$f":"SUM(AN53:AO53)","v":58955999.999999978}]
[null,"Annual Operating Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,500 lb","Grinder mixers and feed mixers",null,null,null,null,null,null,null,null,null,"insurance",{"$f":"E38*0.01","v":1700},{"$f":"E60*0.01","v":0},{"$f":"SUM(AN54:AO54)","v":1700}]
[null,"Repairs and maintenance =",null,"annual repair rate x purchase price",{"$f":"(E38*E42/100)","v":4998},{"$f":"IFERROR(E55/$E$39,0)","v":49.98},{"$f":"IFERROR(F55/($C$15),0)","v":4.9000000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Large size square baler","Bale processors",null,null,null,null,null,null,null,null,null,"repairs",{"$f":"E38*E42/100","v":4998},{"$f":"E60*E64/100","v":0},{"$f":"SUM(AN55:AO55)","v":4998}]
[null,"Total Operating costs",null,null,{"$f":"SUM(E54:E55)","v":4998},49.98,{"$f":"IFERROR(F56/($C$15),0)","v":4.9000000000000004},"(D)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,000 lb/wrapper","Manure spreader",null,null,null,null,null,null,null,null,null,"Total",{"$f":"SUM(AN53,AN54,AN55)","v":58962697.999999978},{"$f":"SUM(AO53,AO54,AO55)","v":0},{"$f":"SUM(AN56:AO56)","v":58962697.999999978},{"$f":"E35+(E35*C81)+E85","v":145076.89287942377},{"$f":"SUM(AP56:AQ56,AN57:AO57)","v":67952179.5928794}]
[null,"Total Implement Costs",null,null,{"$f":"SUM(E56,E52)","v":20397.604669757216},{"$f":"SUM(F56,F52)","v":203.97604669757214},19.99765163701688,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-row forage harvester",null,null,null,null,null,null,null,null,null,null,"profit",{"$f":"AN56*C81","v":8844404.6999999955},{"$f":"AO56*C81","v":0}]
[null,"+ IMPLEMENT 2 (TILLAGE IMPLEMENT, PTO MACHINE, OTHER)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Self-propelled forage harvester, 6 row, 15 ft",null,null,null,null,null,null,null,null,null,null,"per hour",{"$f":"IFERROR(AN56/E39,\"\")","v":589626.97999999975},{"$f":"IFERROR(AO56/E61,\"\")","v":""},null,{"$f":"IFERROR(AQ56/E12,\"\")","v":580.30757151769512},{"$f":"SUM(AN58:AQ58)","v":590207.2875715174}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Large forage blower"]
[null,"Life (years)",{"$f":"IF(D58<>\"\",VLOOKUP(D58,DeprRep,3,FALSE),0)","v":0},"Purchase Price",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6R – 30-in. corn hd",null,null,null,null,null,null,null,null,null,null,"ST rental","implement1","implement2",null,"power"]
[null,"Acres/year",{"$f":"E61*C15","v":0},"Hours per year",{"$f":"IF(D58<>\"\",VLOOKUP(D58,DeprRep,2,FALSE),0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12R – 30-in. corn hd",null,null,null,null,null,null,null,null,null,null,"machine costs",{"$f":"AN56","v":58962697.999999978},{"$f":"AO56","v":0},null,{"$f":"E35-E32","v":95103.8198951511},{"$f":"SUM(AN61:AQ61)","v":59057801.819895126}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grain head 25 ft",null,null,null,null,null,null,null,null,null,null,"profit",{"$f":"AN61*E101","v":8844404.6999999955},{"$f":"AO61*E101","v":0},null,{"$f":"AQ61*E101","v":14265.572984272665},{"$f":"SUM(AN62:AQ62)","v":8858670.2729842681}]
[null,"Trade in Value**",{"$f":"IF(E63=\"\",\"\",E60-(E60*E63/100*C60))","v":0},"Annual depreciation rate (%) from Table 3",{"$f":"IF(D58<>\"\",VLOOKUP(D58,DeprRep,4,FALSE),0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grain head 35 ft",null,null,null,null,null,null,null,null,null,null,"total",{"$f":"SUM(AN61:AN62)","v":67807102.699999973},{"$f":"SUM(AO61:AO62)","v":0},null,{"$f":"SUM(AQ61:AQ62)","v":109369.39287942377},{"$f":"SUM(AR61:AR62)","v":67916472.0928794}]
[null,null,null,"Annual repair rate (%) from Table 3",{"$f":"IF(D58<>\"\",VLOOKUP(D58,DeprRep,5,FALSE),0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"per hour",{"$f":"IFERROR(AN63/E39,\"\")","v":678071.02699999977},{"$f":"IFERROR(AO63/E61,\"\")","v":""},null,{"$f":"IFERROR(AQ63/E12,\"\")","v":437.47757151769508},{"$f":"SUM(AN64:AQ64)","v":678508.50457151746}]
[null,"Annual Fixed Cost",null,null,"Total annual $","$ per hour","$ per acre"]
[null,"Capital recovery*"]
[null,"purchase price – trade-in value",null,{"$f":"(E60-C63)","v":0}]
[null,"capital recovery factor (from Table 4)","x",{"$f":"IFERROR((C5*(1+C5)^C60)/((1+C5)^C60-1),0)","v":0}]
[null,null,null,{"$f":"IFERROR(D67*D68,0)","v":0}]
[null,"trade-in value x annual interest rate**","+",{"$f":"(C63*C5)","v":0}]
[null,"Total capital recovery",null,null,{"$f":"D69+D70","v":0},{"$f":"IFERROR(E71/$E$61,0)","v":0},{"$f":"IFERROR(E71/($E$61*$C$15),0)","v":0}]
[]
[null,"Insurance & housing = ",null,{"$f":"\"purchase price x \"&$C$6*100&\" %\"","v":"purchase price x 1 %"},{"$f":"E60*C6","v":0},{"$f":"IFERROR(E73/$E$61,0)","v":0},{"$f":"IFERROR(E73/($E$61*$C$15),0)","v":0}]
[null,"Total Fixed Cost",null,null,{"$f":"SUM(E67:E73)","v":0},0,{"$f":"IFERROR(E74/($E$61*$C$15),0)","v":0},"(C)"]
[]
[null,"Annual Operating Cost"]
[null,"Repairs and maintenance =",null,"Annual repair rate x purchase price",{"$f":"(E60*E64/100)","v":0},{"$f":"IFERROR(E77/$E$61,0)","v":0},{"$f":"IFERROR(E77/($E$61*$C$15),0)","v":0}]
[null,"Total Operating costs",null,null,{"$f":"SUM(E76:E77)","v":0},0,{"$f":"IFERROR(E78/($E$61*$C$15),0)","v":0},"(D)"]
[null,"Total Implement Costs",null,null,{"$f":"SUM(E78,E74)","v":0},0,{"$f":"IFERROR(E79/($E$61*$C$15),0)","v":0}]
[null," = Annual Machinery Costs  (A+B+C+D) ",null,null,{"$f":"SUM(E79,E35,E57)","v":139801.42456490832},{"$f":"F79+F57+F35","v":681.59132627817655},{"$f":"G79+G57+G35","v":66.822679046880069},"(E)"]
[null,"Return to management, administration costs",{"$f":"E8","v":0.15},"Operator labour (self or hired) per hour  ",{"$f":"E7","v":27}]
[null,null,null,"Labour allowance for machine travel, downtime",0.15]
[null,null,null,null,"Total annual $","$ per hour","$ per acre"]
[null," + Margin (return to management, administration costs)",null,null,{"$f":"E80*C81","v":20970.213684736245},{"$f":"E84/E12","v":83.880854738944976},{"$f":"IFERROR(E84/C12,0)","v":8.2236132097004884},"(F)"]
[null," + Operator labour (self or hired) --- (suggest 15% over machine hour for travel, downtime)  # of machinery hours x 1.15 x wage/hour",null,null,{"$f":"E12*E81*(1+E82)","v":7762.4999999999991},{"$f":"E85/E12","v":31.049999999999997},{"$f":"IFERROR(E85/C12,0)","v":3.0441176470588234},"(G)"]
[null,"=    Total Costs     (E+F+G)",null,null,{"$f":"E80+E84+E85","v":168534.13824964457},null,null,"(H)"]
[null," = Custom Rate ",null,"Per hour",null,{"$f":"F79+F57+F35+F84+F85","v":796.52218101712151}]
[null,null,null,"Per acre",null,null,{"$f":"IFERROR(G79+G57+G35+G84+G85,0)","v":78.090409903639383}]
[null,"* The capital recovery method estimates the annual depreciation and interest costs. It combines depreciation and"]
[null,"interest costs in one calculation. To calculate the capital recovery costs, the capital recovery factor is multiplied by total"]
[null,"depreciation and adds the result of the trade-in value multiplied by the interest rate. Table 4 provides the capital recovery"]
[null,"factors for selected combinations of years and interest rates."]
[null,"** Trade-in value = purchase price – (purchase price x annual depreciation rate (from Table 3) x number of years owned)."]
[null,"*** Interest: Interest calculation is the average annual interest cost of the investment (yours and/or the lender’s) that is tied up in the machine."]
[]
[]
[]
[null,"Short Term Equipment Rental Rate Calculator",null,null,"Total annual $","$ per hour","$ per acre"]
[null," +   Machinery Costs   (from Custom Rate Calculator above)",null,null,{"$f":"E80","v":139801.42456490832},{"$f":"F80","v":681.59132627817655},{"$f":"G80","v":66.822679046880069},"(E)"]
[null," –   Total Fuel and Lubricant cost (if any)  (see Custom Rate Calculator above)",null,null,{"$f":"E32","v":24300},{"$f":"F32","v":97.2},{"$f":"G32","v":9.529411764705884},"(J)"]
[null,"Return to management percentage",null,null,{"$f":"C81","v":0.15}]
[null," + Margin (return to management, admin. costs) suggest 15 % of Machinery Costs ( E – J) x 0.15 ",null,null,{"$f":"(E99-E100)*E101","v":17325.213684736245},{"$f":"(F99-F100)*E101","v":87.65869894172647},{"$f":"(G99-G100)*E101","v":8.593990092326127},"(K)"]
[null,"=    Total Costs    (E–J+K)                                                                                                     ",null,null,{"$f":"E99-E100+E102","v":132826.63824964457},null,null,"(L)"]
[null," = Rental Rate                                  ",null,"Per hour",null,{"$f":"F99-F100+F102","v":672.05002521990298}]
[null,null,null,"Per acre",null,null,{"$f":"G99-G100+G102","v":65.887257374500308}]
[null,"Note:  Rental Rates may have minimum daily or weekly rates"]
[]
[]
[null,"End of worksheet"]

{"sheet":"Tables","index":2,"n_rows":73,"n_cols":28,"rows_kept":73,"cut":false,"hidden":false,"merged":[]}
[null,"Tables 4 and 5 scroll right"]
[]
[null,"Table 3, Annual hours of use, optimal life, depreciation and repair rates",null,null,null,null,null,"Table 4. Capital recovery factors",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TABLE 5. Performance, Horsepower and Fuel Requirements of Selected Farm Equipment"]
[null,"Machine","Annual Use (hours)","Optimal Life (years)","Annual Depreciation Rate (% of purchase price) ","Annual Repair Rate (% of purchase price)",null,null,"Interest rate",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rated Engine HP(1,2)","Acres/hour(2)","Litres/acre","Litres/hour(3)"]
[null,"2WD tractor",300,20,3.3000000000000003,2.31,null,"Year",0.02,0.03,0.04,0.05,0.06,7.0000000000000007E-2,0.08,0.09,0.1,0.11,0.12,0.13,0.14000000000000001,0.15,null,"4–18-in. furrow plow",85,2.8,5.8285714285714292,16.32]
[null,"Front wheel assist tractor",450,15,4.4000000000000004,2.73,null,1,1.02,1.03,1.04,1.05,1.06,1.07,1.08,1.0900000000000001,1.1000000000000001,1.1100000000000001,1.1200000000000001,1.1299999999999999,1.1399999999999999,1.1499999999999999,null,"6–18-in. furrow plow",160,3,10.24,30.72]
[null,"4WD tractor",450,15,4.4000000000000004,2.63,null,2,0.51500000000000001,0.52300000000000002,0.53,0.53800000000000003,0.54500000000000004,0.55300000000000005,0.56100000000000005,0.56799999999999995,0.57599999999999996,0.58399999999999996,0.59199999999999997,0.59899999999999998,0.60699999999999998,0.61499999999999999,null,"8–18-in. furrow plow",285,5.6,9.7714285714285722,54.72]
[null,"Tracked tractor",450,15,4.4000000000000004,3.36,null,3,0.34699999999999998,0.35399999999999998,0.36,0.36699999999999999,0.374,0.38100000000000001,0.38800000000000001,0.39500000000000002,0.40200000000000002,0.40899999999999997,0.41599999999999998,0.42399999999999999,0.43099999999999999,0.438,null,"24-ft field cultivator",160,9,3.4133333333333331,30.72]
[null,"SP Rotary combine",250,12,5.6000000000000005,2.63,null,4,0.26300000000000001,0.26900000000000002,0.27500000000000002,0.28199999999999997,0.28899999999999998,0.29499999999999998,0.30199999999999999,0.309,0.315,0.32200000000000001,0.32900000000000001,0.33600000000000002,0.34300000000000003,0.35,null,"31-ft field cultivator",255,20.6,2.3766990291262133,48.96]
[null,"Rigid headers",250,20,3.3000000000000003,2.1,null,5,0.21199999999999999,0.218,0.22500000000000001,0.23100000000000001,0.23699999999999999,0.24399999999999999,0.25,0.25700000000000001,0.26400000000000001,0.27100000000000002,0.27700000000000002,0.28399999999999997,0.29099999999999998,0.29799999999999999,null,"44-ft field cultivator",305,29.1,2.0123711340206185,58.56]
[null,"Pickup headers",250,20,3.3000000000000003,1.58,null,6,0.17899999999999999,0.185,0.191,0.19700000000000001,0.20300000000000001,0.21,0.216,0.223,0.23,0.23599999999999999,0.24299999999999999,0.25,0.25700000000000001,0.26400000000000001,null,"16-ft chisel plow",175,9,3.7333333333333334,33.6]
[null,"Flex headers",250,15,4.4000000000000004,2.63,null,7,0.155,0.161,0.16700000000000001,0.17299999999999999,0.17899999999999999,0.186,0.192,0.19900000000000001,0.20499999999999999,0.21199999999999999,0.219,0.22600000000000001,0.23300000000000001,0.24,null,"21-ft chisel plow",275,12.6,4.1904761904761907,52.800000000000004]
[null,"Draper headers",250,15,4.4000000000000004,2.94,null,8,0.13700000000000001,0.14199999999999999,0.14899999999999999,0.155,0.161,0.16700000000000001,0.17399999999999999,0.18099999999999999,0.187,0.19400000000000001,0.20100000000000001,0.20799999999999999,0.216,0.223,null,"24-ft tandem disk",170,15.1,2.16158940397351,32.64]
[null,"Corn headers",100,15,4.4000000000000004,2.94,null,9,0.123,0.128,0.13400000000000001,0.14099999999999999,0.14699999999999999,0.153,0.16,0.16700000000000001,0.17399999999999999,0.18099999999999999,0.188,0.19500000000000001,0.20200000000000001,0.21,null,"30-ft tandem disk",255,15.3,3.1999999999999997,48.96]
[null,"SP Swather",200,15,4.4000000000000004,2.1,null,10,0.111,0.11700000000000001,0.123,0.13,0.13600000000000001,0.14199999999999999,0.14899999999999999,0.156,0.16300000000000001,0.17,0.17699999999999999,0.184,0.192,0.19900000000000001,null,"10-ft offset disk",125,6,4,24]
[null,"Grain carts",250,20,3.3000000000000003,2.1,null,11,0.10199999999999999,0.108,0.114,0.12,0.127,0.13300000000000001,0.14000000000000001,0.14699999999999999,0.154,0.161,0.16800000000000001,0.17599999999999999,0.183,0.191,null,"16-ft offset disk",175,9.6,3.5000000000000004,33.6]
[null,"Powered augers",100,20,3.3000000000000003,1.58,null,12,9.5000000000000001E-2,0.1,0.107,0.113,0.11899999999999999,0.126,0.13300000000000001,0.14000000000000001,0.14699999999999999,0.154,0.161,0.16900000000000001,0.17699999999999999,0.184,null,"21-ft vertical tillage",215,19.600000000000001,2.1061224489795918,41.28]
[null,"PTO augers",100,20,3.3000000000000003,1.58,null,13,8.7999999999999995E-2,9.4E-2,0.1,0.106,0.113,0.12,0.127,0.13400000000000001,0.14099999999999999,0.14799999999999999,0.156,0.16300000000000001,0.17100000000000001,0.17899999999999999,null,"30-ft vertical tillage",305,27.2,2.1529411764705886,58.56]
[null,"Grain vac",50,15,4.4000000000000004,2.1,null,14,8.3000000000000004E-2,8.8999999999999996E-2,9.5000000000000001E-2,0.10100000000000001,0.108,0.114,0.121,0.128,0.13600000000000001,0.14299999999999999,0.151,0.159,0.16700000000000001,0.17499999999999999,null,"43-ft vertical tillage",420,39.200000000000003,2.0571428571428569,80.64]
[null,"SP Forage harvester",400,10,6.7,8.4,null,15,7.8E-2,8.4000000000000005E-2,0.09,9.6000000000000002E-2,0.10299999999999999,0.11,0.11700000000000001,0.124,0.13100000000000001,0.13900000000000001,0.14699999999999999,0.155,0.16300000000000001,0.17100000000000001,null,"12-row strip tillage",330,17.5,3.6205714285714286,63.36]
[null,"SP Forage harvester header",400,10,6.7,8.4,null,16,7.3999999999999996E-2,0.08,8.5999999999999993E-2,9.1999999999999998E-2,9.9000000000000005E-2,0.106,0.113,0.12,0.128,0.13600000000000001,0.14299999999999999,0.151,0.16,0.16800000000000001,null,"6R – 30-in. row crop planter",110,7.6,2.7789473684210528,21.12]
[null,"SP Mower/conditioner",150,15,4.4000000000000004,3.36,null,17,7.0000000000000007E-2,7.5999999999999998E-2,8.2000000000000003E-2,8.8999999999999996E-2,9.5000000000000001E-2,0.10199999999999999,0.11,0.11700000000000001,0.125,0.13200000000000001,0.14000000000000001,0.14899999999999999,0.157,0.16500000000000001,null,"12R – 30-in. row crop planter",160,15.3,2.0078431372549019,30.72]
[null,"PT Mower/conditioner (sickle)",150,15,4.4000000000000004,2.1,null,18,6.7000000000000004E-2,7.2999999999999995E-2,7.9000000000000001E-2,8.5999999999999993E-2,9.1999999999999998E-2,9.9000000000000005E-2,0.107,0.114,0.122,0.13,0.13800000000000001,0.14599999999999999,0.155,0.16300000000000001,null,"16R – 30-in. row crop planter",175,20.399999999999999,1.6470588235294119,33.6]
[null,"PT Mower/conditioner (disc)",150,15,4.4000000000000004,2.63,null,19,6.4000000000000001E-2,7.0000000000000007E-2,7.5999999999999998E-2,8.3000000000000004E-2,0.09,9.7000000000000003E-2,0.104,0.112,0.12,0.128,0.13600000000000001,0.14399999999999999,0.153,0.161,null,"6R – 30-in. minimum-till planter",85,6.4,2.5499999999999998,16.32]
[null,"Hay rake (wheel)",50,20,3.3000000000000003,2,null,20,6.0999999999999999E-2,6.7000000000000004E-2,7.3999999999999996E-2,0.08,8.6999999999999994E-2,9.4E-2,0.10199999999999999,0.11,0.11700000000000001,0.126,0.13400000000000001,0.14199999999999999,0.151,0.16,null,"12R – 30-in. minimum-till planter",175,15.3,2.1960784313725492,33.6]
[null,"Round baler",100,15,4.4000000000000004,1.58,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16R – 30-in. minimum-till planter",255,20.399999999999999,2.4000000000000004,48.96]
[null,"Large square baler",150,15,4.4000000000000004,1.79,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25-ft grain drill",160,11.7,2.6256410256410256,30.72]
[null,"Small square baler",100,20,3.3000000000000003,1.05,null,"Tractor example using Table 3 and 4:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"35-ft grain drill",255,16.3,3.003680981595092,48.96]
[null,"PT round bale mover",100,15,4.4000000000000004,2.63,null,null,"310 Horsepower (HP) Four Wheel Drive (4WD) Tractor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-ft presswheel drill",85,5.0999999999999996,3.2,16.32]
[null,"PT large square bale mover",200,20,3.3000000000000003,2.1,null,"Purchase price",470000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-ft presswheel drill",160,8.5,3.6141176470588232,30.72]
[null,"SP small square bale mover",150,15,4.4000000000000004,2.63,null,"Projected use","450 hr per year for 5 years",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"15-ft no-till drill",160,7,4.3885714285714288,30.72]
[null,"Air drills (independent openers)",200,15,4.4000000000000004,3.68,null,"Depreciaton","Estimated total depreciation over the 5 years:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-ft no-till drill",200,9.3000000000000007,4.129032258064516,38.4]
[null,"Air hoe drills",200,15,4.4000000000000004,3.15,null,null,"= 4.4% annual depreciation rate (from Table 3, 4WD tractors) x 5 years x $470,000 = $103,400 total depreciation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"90-ft sprayer, pull type",110,49.6,0.42580645161290326,21.12]
[null,"Air disk drills",200,15,4.4000000000000004,3.15,null,"Trade-in value","= $470,000 (purchase price) – $103,400 (total depreciation) = $366,600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"90-ft sprayer, self propelled",95,72.5,0.25158620689655176,16.3]
[null,"Air seeder",200,15,4.4000000000000004,3.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"9-ft mower conditioner",45,4.4000000000000004,1.9636363636363636,8.64]
[null,"Row crop planters",100,10,6.7,4.2,null,"Capital recovery:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"13-ft rotary mower/conditioner",85,9.6999999999999993,1.682474226804124,16.32]
[null,"Plows",100,20,3.3000000000000003,3.68,null,null,"= (total depreciation x capital recovery factor)+ (trade-in value x interest rate)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Square baler",45,4.4000000000000004,1.9636363636363636,8.64]
[null,"Disks",100,20,3.3000000000000003,1.58,null,null,"= ($103,400 x 0.218 (from Table 5, 3% interest and 5 years)) + ($366,600 x 3%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,000 lb",70,3,4.4799999999999995,13.44]
[null,"Cultivators",200,20,3.3000000000000003,1.58,null,null,"= $22,541 + $10,998",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,500 lb",70,4,3.36,13.44]
[null,"Standard harrows",75,25,2.7,1.26,null,null,"= $33,539 per year capital recovery (depreciation and interest costs).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Large size square baler",160,16.3,1.8846625766871163,30.72]
[null,"Heavy harrows",100,20,3.3000000000000003,1.58,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Round baler 1,000 lb/wrapper",70,3,4.4799999999999995,13.44]
[null,"Harrow packers",200,25,2.7,0.53,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-row forage harvester",160,1.4,21.942857142857143,30.72]
[null,"Vertical tillage tools",100,20,3.3000000000000003,3.68,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Self-propelled forage harvester, 6 row, 15 ft",625,5.0999999999999996,20.6,105]
[null,"Land roller",75,20,3.3000000000000003,1.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Large forage blower",70,"—","—",13.44]
[null,"Land scraper",80,10,6.7,2.63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine 6R – 30-in. corn hd",275,5.0999999999999996,11.858823529411767,52.8]
[null,"High clearance sprayers",175,8,8.3000000000000007,3.68,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine 12R – 30-in. corn hd",375,10.199999999999999,8.0000000000000018,72]
[null,"Post pounder",40,20,3.3000000000000003,2.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine grain head 25 ft",375,7.4,11.027027027027028,72]
[null,"Vertical feed mixer",200,15,4.4000000000000004,2.63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combine grain head 35 ft",375,10.4,7.8461538461538467,72]
[null,"Grinder mixers and feed mixers",200,15,4.4000000000000004,3.15,null,"End of worksheet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. Multiply Engine Horsepower by 0.88 to arrive at PTO horsepower"]
[null,"Bale processors",200,15,4.4000000000000004,3.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2. Source: Illinois Machinery Cost Estimates for 2023, University of Illinois, Department of Agricultural and Consumer Economics, 2023."]
[null,"Manure spreader",100,10,6.7,4.62,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3. Source: Nebraska Tractor Test Laboratory, 2018–2024. Tractor fuel consumption results."]
[null,"Source: Farm Machinery Custom and Rental Rate Guide, Saskatchewan Ministry of Agriculture, 2024-25"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"End of worksheet"]
[]
[]
[null,"EXAMPLE ","Accumulated Repair Cost Calculation "]
[null,"New 425 HP combine with corn header","$820,000 = $740,000 (combine) + $ 170,000 (corn header)"]
[null,"Estimated annual repair rates","2.63% combine"]
[null,null,"2.94% corn head"]
[null,"from Table 3"]
[null,"Estimated annual repair costs","Combine: $740,000 x 2.63% for an average of $19,462/year"]
[null,null,"Corn header: $170,000 x 2.94% for an average of $4,998/year"]
[]
[null,null,"Total annual repair costs = $19,462 + $4,998 = $24,460 per year"]
[null,"Used Machinery","When calculating the depreciation on used machinery, use the actual price paid "]
[null,null,"for the machine minus its expected trade-in or salvage value, divided by the "]
[null,null,"expected life of the machine on your farm. Increase repair rates to levels "]
[null,null,"appropriate for the age or number of hours on the machine. Expect to have "]
[null,null,"higher than normal repair expenses in the first year of ownership of a"]
[null,null," used machine as you bring it back into top operating shape"]
[]
[null,"End of worksheet"]

{"sheet":"Factsheet","index":3,"n_rows":11,"n_cols":1,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["GUIDE TO CUSTOM FARMWORK AND SHORT-TERM EQUIPMENT RENTAL "]
["by John Molenhuis"]
["Business Analysis and Cost of Production Program Specialist"]
["Policy Division,"]
["Ontario Ministry of Agriculture, Food and Agribusiness"]
[]
[" This factsheet contains the 2024 Survey of Custom Farmwork Rates charged in Ontario and a guide to writing custom farmwork agreements."]
[]
["https://www.ontario.ca/page/cost-production-crops-and-livestock "]
[]
["End of worksheet"]

{"sheet":"2024Rates","index":4,"n_rows":375,"n_cols":20,"rows_kept":375,"cut":false,"hidden":false,"merged":[[220,5,220,6],[219,8,219,9],[219,10,219,11],[248,5,248,6],[222,1,222,2],[247,8,247,9],[247,10,247,11],[0,1,0,19],[1,1,1,19],[2,1,2,19],[3,1,3,19],[113,1,113,2],[113,8,113,9],[113,10,113,11],[113,12,113,13],[54,16,54,17],[55,5,55,6],[54,1,54,2],[54,3,54,7],[92,5,92,6],[57,1,57,2],[113,16,113,17],[53,1,53,19],[250,1,250,2],[114,5,114,6],[91,14,91,15],[91,16,91,17],[157,16,157,17],[158,5,158,6],[157,8,157,9],[157,10,157,11],[157,12,157,13],[157,14,157,15],[91,8,91,9],[91,10,91,11],[91,12,91,13],[113,14,113,15],[160,1,160,2],[247,14,247,15],[307,5,307,6],[306,1,306,2],[306,8,306,9],[306,10,306,11],[306,12,306,13],[219,18,219,19],[247,18,247,19],[306,18,306,19],[365,18,365,19],[365,12,365,13],[365,14,365,15],[365,16,365,17],[306,14,306,15],[306,16,306,17],[219,12,219,13],[219,14,219,15],[247,16,247,17],[219,16,219,17],[247,12,247,13],[54,18,54,19],[91,18,91,19],[113,18,113,19],[157,18,157,19],[116,1,116,2],[117,1,117,2],[54,14,54,15],[54,8,54,9],[54,10,54,11],[54,12,54,13],[366,5,366,6],[365,8,365,9],[365,10,365,11],[309,1,309,2],[368,1,368,2]]}
[null,"Survey of Ontario Custom Farmwork Rates"]
[null,"charged in 2024"]
[null,"John Molenhuis, OMAFA,  Business Analysis and Cost of Production Specialist"]
[null,"Infosheet"]
[null,"Survey Details"]
[null,"Survey results of rates charged in 2024 by 200 Ontario custom farmwork operators are summarized on a provincial basis and also by regional areas. The survey received insufficient responses for Area 6. Where available the provincial average 2021 rates are also listed. The 2021 survey is the previous survey to the 2024 survey. "]
[]
[null,"Average Rates "]
[null,"An average rate is given when there are at least 3 reports. The greater the number of reports, the greater the summary reflects the market rates. "]
[null,"The # column indicates the number of responses received for the operation."]
[]
[null,"What are percentiles and how can you use them?"]
[null,"Percentiles have been used to help show the range of the rates that were charged. For example, in the Provincial Summary, the 15th percentile for corn combining is $54/acre and the 85th percentile is $75/acre. This means that 15% of those surveyed charged $54/acre or less and 15% charged more than $75. Seventy percent (85th –15th percentile) of all those reporting charged between $54 and $75/acre. The average rate charged was $65/acre."]
[]
[null,"Survey Areas"]
[]
[null,"Area 1"]
[null,"Chatham-Kent, Elgin, Essex, Lambton, Middlesex"]
[null,"Area 2"]
[null,"Brant, Haldimand, Hamilton, Niagara, Norfolk, Oxford"]
[null,"Area 3"]
[null,"Bruce, Dufferin, Grey, Halton, Huron, Peel, Perth, Simcoe, Waterloo, Wellington "]
[null,"Area 4"]
[null,"Durham, Haliburton, Hastings, Kawartha Lakes, Muskoka, Northumberland, Parry Sound, Peterborough, Prince Edward, York"]
[null,"Area 5"]
[null,"Frontenac, Lanark, Leeds-Grenville, Lennox-Addington, Ottawa, Prescott-Russell, Renfrew, Stormont-Dundas-Glengarry"]
[null,"Area 6"]
[null,"Algoma, Cochrane, Kenora, Manitoulin, Nipissing, Rainy River, Sudbury, Thunder Bay, Timiskaming "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Survey of Custom Farmwork Rates charged in 2024"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"TILLAGE"]
[null,"Moldboard Plow - fixed furrow","ac.",14,37.571428571428569,29.75,44.3,36.694444444444443,5,40.200000000000003,"","",7,33.285714285714285,"","","","","",""]
[null,null,"hr.","","",122.49999999999999,227.5,165.33333333333334,"","","","","","","","","","","",""]
[null,"Moldboard Plow - rollover","ac.",4,39.5,"","",38.25,"","","","","","","","","","","",""]
[null,null,"hr.",4,136.25,"","","","","","","",3,123.33333333333333,"","","","","",""]
[null,"Moldboard Plow - variable width","ac.",7,40.428571428571431,"","",33.694444444444443,"","","","",5,40.6,"","","","","",""]
[null,null,"hr.",3,203.33333333333334,"","",91.666666666666671,"","","","",3,203.33333333333334,"","","","","",""]
[null,"Chisel Plow/Soil Saver","ac.",48,33.78125,25,41.899999999999991,28.681034482758619,10,39,12,34,19,29.973684210526315,"","",7,36.285714285714285,"",""]
[null,null,"hr.",4,225,"","",230.5,"","","","",3,233.33333333333334,"","","","","",""]
[null,"Disc -Primary tillage","ac.",40,27.962499999999999,22.549999999999997,35,24.46875,10,25.3,7,28,14,27.642857142857142,"","",7,30.071428571428573,"",""]
[null,null,"hr.","","",250,250,169,"","","","","","","","","","","",""]
[null,"Disc -Secondary tillage","ac.",25,27.24,19.2,35,22.75,4,23.75,6,24.75,8,27.5,"","",5,28.7,"",""]
[null,null,"hr.",4,193.75,"","",167,"","","","",3,208.33333333333334,"","","","","",""]
[null,"Disc - High Speed","ac.",54,30.00925925925926,25,35,23.940789473684209,13,28.46153846153846,8,31.4375,22,29.727272727272727,3,30.333333333333332,7,32.714285714285715,"",""]
[null,null,"hr.","","","","",547,"","","","","","","","","","","",""]
[null,"Vertical tillage","ac.",47,27.957446808510639,23.799999999999997,35,23.614035087719298,15,26.4,9,28.333333333333332,15,27.533333333333335,3,33.333333333333336,5,30,"",""]
[null,null,"hr.","","","","",252.75,"","","","","","","","","","","",""]
[null,"Strip tillage","ac.",9,39.333333333333336,30,43.6,29.4,"","","","",6,34.166666666666664,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"V ripping","ac.",10,37.35,30.449999999999996,42.599999999999994,37.571428571428569,6,36.833333333333336,"","","","","","","","","",""]
[null,null,"hr.","","",300,300,"","","","","","","","","","","","",""]
[null,"Field Cultivate","ac.",86,23.255813953488371,16.5,30,18.144186046511628,18,24.194444444444443,21,22.714285714285715,33,20.787878787878789,3,25,11,29.681818181818183,"",""]
[null,null,"hr.",5,182,"","",265.88888888888891,"","","","",4,190,"","","","","",""]
[null,"Harrowing","ac.",5,17,"","",12.6,"","","","",4,15,"","","","","",""]
[null,null,"hr.","","",450,450,"","","","","","","","","","","","",""]
[null,"Deep tillage/Subsoiling","ac.",18,39.962962962962962,35,50,30.25,8,40.916666666666664,"","",6,35.333333333333336,"","",3,48.333333333333336,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Soil finisher","ac.",3,29.333333333333332,"","",21.142857142857142,3,29.333333333333332,"","","","","","","","","",""]
[null,null,"hr.","","",250,250,"","","","","","","","","","","","",""]
[null,"Packer/Rolling","ac.",56,10.696428571428571,6.25,14,9.0809090909090902,6,10.5,10,11.125,29,9.9913793103448274,3,12,8,12.375,"",""]
[null,null,"hr.",3,150,"","",193.33333333333334,"","","","","","","","","","","",""]
[null,"Stalk Chopping","ac.",3,24.666666666666668,"","",27,3,24.666666666666668,"","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Survey of Custom Farmwork Rates charged in 2024"]
[null,"PLANTING",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,"SOYBEANS",null,"# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,"Unit",null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"Conventional Row Planter - 15/20\"","ac.",47,32.106382978723403,28,37,26.745238095238093,19,31,14,32.142857142857146,12,33.75,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Conventional Row Planter - 30\"","ac.",25,33.24,28,40,26.378947368421052,6,30.166666666666668,"","",10,31.8,"","",6,36.166666666666664,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Minimum/No-Till Planter - 15/20\"","ac.",54,32.018518518518519,26.9,37,27.871794871794872,15,31.4,12,31.25,21,31.80952380952381,"","",6,36.166666666666664,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Minimum/No-Till Planter - 30\"","ac.",10,34.799999999999997,32.35,36.65,28.071428571428573,"","","","",6,34.333333333333336,3,36.666666666666664,3,35,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Strip tillage planter - 15/20\"","ac.",3,35,"","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Strip tillage planter - 30\"","ac.","","",36,36,25.400000000000002,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Conventional Drill","ac.",14,31.142857142857142,24.85,37.049999999999997,22.8,"","",3,28.333333333333332,9,31,"","","","","",""]
[null,null,"hr.","","",22.25,32.75,"","","","","","","","","","","","",""]
[null,"No-Till Drill","ac.",54,32.537037037037038,27.95,36.024999999999999,27.532608695652176,9,30.444444444444443,9,32.611111111111114,22,31.65909090909091,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Air Seeder","ac.",56,32.896428571428572,28,36.875,26.340425531914892,6,30.833333333333332,11,33.409090909090907,28,31.775000000000002,9,35.555555555555557,5,34.6,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"PLANTING"]
[null,"CORN"]
[null,"Conventional Row Planter - 15/20 \"","ac.",6,34.25,"","",30.125,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Conventional Row Planter - 30\"","ac.",92,32.747282608695649,28,39.349999999999994,26.602409638554217,18,31.666666666666668,19,32.263157894736842,39,32.121794871794869,5,41,11,33.81818181818182,"",""]
[null,null,"hr.","","","","",451.6,"","","","","","","","","","","",""]
[null,"Minimum/No-Till - 15/20\"","ac.",4,32.75,"","",29.25,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Minimum/No-Till - 30\"","ac.",50,34.14,28,40,28.407894736842106,8,30.125,9,33.666666666666664,22,32.75,6,40.75,4,40.75,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Strip Tillage - 15/20\"","ac.","","",34.15,34.85,"","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Strip Tillage - 30\"","ac.",7,41.714285714285715,"","",26.676923076923078,3,46,"","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"No-Till Drill","ac.",4,32.5,"","",33.333333333333336,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Air Seeder","ac.",4,32.75,"","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"CEREALS (OATS, BARLEY, WHEAT)"]
[null,"Conventional Drill","ac.",23,32.304347826086953,25,37.4,22.431818181818183,4,30.75,7,31.714285714285715,10,31,"","","","","",""]
[null,null,"hr.","","",81.75,113.25,112.5,"","","","","","","","","","","",""]
[null,"No-Till Drill","ac.",44,32.159090909090907,25.9,36.549999999999997,26.990384615384617,9,29.333333333333332,6,29.833333333333332,20,31.574999999999999,7,38.071428571428569,"","","",""]
[null,null,"hr.","","","","",226.66666666666666,"","","","","","","","","","","",""]
[null,"Air Seeder","ac.",54,33.220370370370375,29.9,36.024999999999999,26.439024390243901,7,31.571428571428573,12,34.179166666666667,26,33.028846153846153,"","",6,34.166666666666664,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"FORAGES"]
[null,"Drill - single tank","ac.",11,29.545454545454547,23.5,35,24.2,"","",4,30.5,3,28.333333333333332,"","","","","",""]
[null,null,"hr.","","",75,75,"","","","","","","","","","","","",""]
[null,"Drill - multiple products","ac.",10,34.700000000000003,30.449999999999996,38,27.57,"","",3,34.333333333333336,4,34,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Brillion Type","ac.","","",20,20,"","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Broadcast/ATV Spreading","ac.",10,9.5,6.1749999999999998,10,5.8166666666666664,"","",3,8.1666666666666661,5,11.2,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Frost seeding","ac.",4,12.5,"","","","","","","",3,13.333333333333334,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Cover crop planting","ac.",21,30.547619047619047,20,40,23.153846153846153,3,30.333333333333332,5,32.200000000000003,7,28.142857142857142,3,27.833333333333332,3,36.333333333333336,"",""]
[null,null,"hr.","","",120,120,"","","","","","","","","","","","",""]
[]
[]
[null,"Survey of Custom Farmwork Rates charged in 2024"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"WEED CONTROL"]
[null,"HERBICIDE (excluding herbicide cost)"]
[null,"Pull-type Sprayer","ac.",17,13.235294117647058,10,15,10.952380952380953,3,14,3,13,6,11.833333333333334,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null," Self Propelled","ac.",70,13.595000000000001,12,15,10.96326530612245,16,13.903124999999999,16,13.15625,24,13.09375,4,16.125,9,14.438888888888888,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null," Self Propelled  High Clearance\n Sprayer","ac.",58,14.322413793103449,12,16,10.90625,16,13.496874999999999,10,16.649999999999999,26,14.028846153846153,3,15.166666666666666,"","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Rope Wick","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Spray tassled corn (high water volume)","ac.",32,16.443750000000001,14,18.699999999999996,13.685416666666667,8,15.99375,5,17.2,15,16.283333333333335,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"MECHANICAL"]
[null,"Inter-row cultivation","ac.","","",21.799999999999997,30.200000000000003,14.625,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Rotary Hoe","ac.","","",15.75,19.25,17.333333333333332,null,null,"","","","","","","","","",""]
[null,null,"hr.","","",85,85,"","","","","","","","","","","","",""]
[null,"Scuffler","ac.","","",20,20,"","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Weed zapper","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Flame weeder","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"FERTILIZER APPLICATION"]
[null,"Spread dry fertilizer","ac.",44,13.254545454545456,10.612500000000001,15,10.407999999999999,10,13.094999999999999,10,13.55,15,13.85,4,13,4,12.25,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Spread dry fertilizer - in crop high clearance","ac.",8,15.21875,11.762499999999999,16.95,11.25,"","","","",4,16.4375,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Rental of dry bulk applicator","ac.","","","","","","","","","","","","","","","","",""]
[null,"Rental of dry bulk applicator","mt.",8,18.1875,15,20.95,14,4,16.375,"","",4,20,"","","","","",""]
[null,"Side-dress Dry fertilizer","ac.",4,22.375,"","",14.375,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Anhydrous","ac.",4,13.25,"","",20,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Liquid -  ground/top dress","ac.",16,15.590624999999999,13.237500000000001,19.5,11.083333333333334,6,16.158333333333335,3,15.166666666666666,3,17,"","",4,14,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Liquid side -dress","ac.",25,17.48,14,22,14.952380952380953,13,18.076923076923077,5,18.8,4,16.5,"","",3,14,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Liquid drop hose, high clearance/late application","ac.",14,18.071428571428573,14.95,18.349999999999994,15.328571428571427,"","","","",8,17.5,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"NDVI sensing w/application (Greenseeker)","ac.","","",16.95,16.95,"","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"SOIL AND MAPPING"]
[null,"Prescription map service","ac.",3,4.666666666666667,"","",3.69,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Elevation mapping","ac.",3,11,"","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Electrical conductivity","ac.","","",5,5,"","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"High resolution mapping","ac.","","",50,50,"","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Grid sampling","ac.",4,8.75,"","",5.3125,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"NDVI Mapping","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Site specific soil sampling","ac.","","",10.049999999999995,42.95,8,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[]
[null,"Survey of Custom Farmwork Rates charged in 2024"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"COMBINING "]
[null,"Corn","ac.",87,65,53.8,75,50.617924528301884,21,63.238095238095241,12,67.083333333333329,35,66.257142857142853,6,57.333333333333336,12,67.833333333333329,"",""]
[null,null,"hr.","","",180,180,365.25,"","","","","","","","","","","",""]
[null,"Corn with chopping corn head","ac.",49,72.83163265306122,60.4,85,55.089285714285715,5,64.400000000000006,15,71.933333333333337,17,76.57352941176471,"","",10,71.099999999999994,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[]
[null,"Soybeans","ac.",133,64.46616541353383,52,75,50.024822695035461,33,57.909090909090907,24,67.25,50,66.14,7,64.285714285714292,18,69.555555555555557,"",""]
[null,null,"hr.","","",260,260,512,"","","","","","","","","","","",""]
[null,"Cereals with chopper","ac.",30,66.266666666666666,52.7,83.25,50.521739130434781,8,57.875,6,71.166666666666671,12,69.833333333333329,"","","","","",""]
[null,null,"hr.","","",165.25,189.75,"","","","","","","","","","","","",""]
[null,"Cereals without chopper","ac.",93,65.053763440860209,53.599999999999994,75,49.525641025641029,22,58,21,68.333333333333329,34,66.235294117647058,5,69,11,67.454545454545453,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Canola","ac.",10,68.3,50,91.499999999999986,51,4,58.25,"","",4,86.25,"","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Grain buggy alone","ac.",8,6.875,5,7.95,7.5714285714285712,"","","","",4,6.25,"","","","","",""]
[null,null,"hr.",7,131.42857142857142,"","",120.2,"","","","",3,140,"","",3,133.33333333333334,"",""]
[null,null,"mt.","","",0,0,null,"","","","","","","","","","","",""]
[null,null,"bu.","","",0,0,null,"","","","","","","","","","","",""]
[null,"Hauling from the field to elevator","bu.","","",0.25,0.25,0.16,"","","","","","","","","","","",""]
[null,"Hauling from the field to elevator","mt.",33,9.2181818181818187,6.92,10.199999999999999,8.415909090909091,5,8.1,8,8.4124999999999996,13,9.1230769230769226,3,12.733333333333334,3,9.8666666666666671,"",""]
[null,null,"ton",33,8.3801652892561975,6.290909090909091,9.2727272727272716,7.6508264462809903,5,7.3636363636363624,8,7.6477272727272716,13,8.2937062937062933,3,11.575757575757576,3,8.9696969696969688,"",""]
[null,null,"mi.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.",8,151.875,85.75,246.5,105,"","",3,120,3,211.66666666666666,"","","","","",""]
[]
[null,"Survey of Custom Farmwork Rates charged in 2024"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"OTHER CROP HARVESTING"]
[null,"Grain swathing","ac.",3,22.333333333333332,"","",22.333333333333332,"","","","","","","","","","","",""]
[null,null,"hr.","","",95.75,99.25,125,"","","","","","","","","","","",""]
[null,"HIGH MOISTURE CORN"]
[null,"    Combine and hauled to silo","ac.",11,66.63636363636364,55,79,50,3,54,3,71,"","","","","","","",""]
[null,null,"hr.","","","","",343.33333333333331,"","","","","","","","","","","",""]
[null,"Combine, grind, haul, blow/pack","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"EDIBLE BEANS"]
[null," Bean Pulling + windrowing","ac.",3,48.833333333333336,"","",48,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Combining -Conventional Grain type","ac.",48,67.6875,55.25,80,54.75,8,58.75,10,72,24,69.833333333333329,4,62.5,"","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Combining -Specialty -Bob/Lilliston ","ac.",4,85.75,"","",67.5,"","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"TRUCKING"]
[null,"Grains and Oilseeds - local ","bu.",4,0.26,"","",0.13999999999999999,4,0.26,"","","","","","","","","",""]
[null,null,"mt.",60,10.704000000000001,8,13.149999999999999,9.5830882352941149,9,9.1666666666666661,10,9.6739999999999995,26,9.865384615384615,6,14.5,8,13.6875,"",""]
[null,null,"ton",60,9.7309090909090905,7.2727272727272725,11.954545454545451,8.711898395721926,9,8.3333333333333339,10,8.7945454545454531,26,8.9685314685314683,6,13.18181818181818,8,12.443181818181817,"",""]
[null,"FORAGE HARVESTING"]
[null,"HAY"]
[null,"Mowing","ac.",8,22.25,20,25,18.90909090909091,"","","","",3,21.666666666666668,"","","","","",""]
[null,null,"hr.","","",400,400,"","","","","","","","","","","","",""]
[null,"Swathing/Conditioning","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Disc bine","ac.",10,23.2,19.350000000000001,30,19.600000000000001,"","","","",5,19.8,3,26.333333333333332,"","","",""]
[null,null,"hr.","","",183,197,236.66666666666666,"","","","","","","","","","","",""]
[null,"Disc bine with conditioner","ac.",16,23.4375,20,25.75,19.685185185185187,3,26.666666666666668,"","",10,22.6,"","","","","",""]
[null,null,"hr.",6,177.5,"","",146.4,"","","","","","","","","","","",""]
[null,"Raking","ac.",21,13.976190476190476,10,18,12.404761904761905,4,14.5,"","",10,14.3,3,14,"","","",""]
[null,null,"hr.",3,128.33333333333334,"","",95,"","","","",3,128.33333333333334,"","","","","",""]
[null,"Tedding","ac.",10,15.25,12,21.899999999999991,12.153846153846153,"","","","",5,15.8,"","","","","",""]
[null,null,"hr.","","",150,150,"","","","","","","","","","","","",""]
[null,"Windrow merging","ac.",10,19.600000000000001,15.7,23.949999999999996,15.833333333333334,"","","","",4,19.25,"","",3,20,"",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"Bale - sm. square (ground)","bale","","",1,1,"","","","","","","","","","","","",""]
[null,"Bale - sm. square (loaded)","bale",6,1.5166666666666666,"","",1.0166666666666666,"","","","","","","","","","","",""]
[null,"Bale - lg. Square  ","ft.",17,1.8205882352941176,1.38,2.15,1.5579365079365077,"","",4,2,7,1.6785714285714286,"","",4,2.0499999999999998,"",""]
[null,"Bale - lg. Square  State +/- 1000 lbs or per ft high density","ft.",5,2.39,"","",1.7277777777777779,"","","","",3,2.3333333333333335,"","","","","",""]
[null,"Bale - lg. Round under 1000 lbs.","bale",11,10,9,11,9.7142857142857135,"","","","",4,9.5,"","","","","",""]
[null,"Bale - lg. Round over 1000 lbs.","bale",14,11.321428571428571,9.9499999999999993,14.049999999999999,9.5500000000000007,"","","","",6,10.75,"","","","","",""]
[null,"Additional chopping",null,"","","","","","","","","","","","","","","","",""]
[null,"Additional chopping","hr.","","",645,645,536.66666666666663,"","","","","","","","","","","",""]
[null,"Entire operation (mowing to baling)  lg. bale",null,"","","","","","","","","","","","","","","","",""]
[null,"Baling corn stalks","bale",6,15.583333333333334,"","",12.375,"","","","",5,15.3,"","","","","",""]
[null,"BALE WRAPPING"]
[null,"Individual -with plastic","bale",5,13.5,"","",7.25,"","","","","","","","","","","",""]
[null,"Tube","bale",11,9.0681818181818183,5.875,11,7.5909090909090908,"","","","",6,8.8333333333333339,4,9.1875,"","","",""]
[null,"Hauling hay bales","bale","","","","","","","","","","","","","","","","",""]
[null,"STRAW  ",null,null,null,null,null,null,"","","","","","","","","","","",""]
[null,"Bale - sm. square (loaded)","bale","","","","","","","","","","","","","","","","",""]
[null,"Bale - lg. Square                             per ft.",null,9,2.1222222222222218,1.83,2.4700000000000002,"","","","","",4,2.0375000000000001,"","","","","",""]
[null,"Bale - lg. Round ","bale",9,11.055555555555555,8.4,12.8,10,"","","","",6,9.9166666666666661,"","","","","",""]
[null,"Bale - lg. Round with netting","bale","","","","","","","","","","","","","","","","",""]
[null,"Survey of Custom Farmwork Rates charged in 2024"]
[]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"HAYLAGE"]
[null,"PT0 Harvester/haul/blow or pack","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"PTO harvester only","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","",360,360,"","","","","","","","","","","","",""]
[]
[null,"Self Propelled Harvester/ Hauling/Blow or Pack","ac.","","","","","","","","","","","","","","","","",""]
[null,"Self Propelled Harvester/ Hauling/Blow or Pack","hr.",8,804.375,556.25,998.5,606.66666666666663,"","","","","","","","","","","",""]
[null,"Self propelled Harvester only","ac.","","","","","","","","","","","","","","","","",""]
[null,"Self propelled Harvester only","hr.",9,655,510,700,455.625,"","",3,615,3,616.66666666666663,"","","","","",""]
[null,"Hauling only - trucks","ac.","","","","","","","","","","","","","","","","",""]
[null,"Hauling only - trucks","hr.",4,126.25,"","",141.66666666666666,"","","","","","","","","","","",""]
[null,"Hauling only - wagons","ac.","","","","","","","","","","","","","","","","",""]
[null,"Hauling only - wagons","hr.",7,138.57142857142858,"","",149.28571428571428,"","","","","","","","",3,138.33333333333334,"",""]
[null,"Packing only","hr.",5,169.5,"","",162.85714285714286,"","",3,174.16666666666666,"","","","","","","",""]
[null,"Blowing only","hr.",3,111.66666666666667,"","","","","","","","","","","","","","",""]
[null,"CORN SILAGE"]
[null,"PT0 Harvester/haul/blow or pack","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","","","","","","","","","","","","","","","",""]
[null,"PTO Harvester only","ac.","","","","","","","","","","","","","","","","",""]
[null,null,"hr.","","",150,150,"","","","","","","","","","","","",""]
[]
[null,"Self Prop Harvester/hauling/blow or pack","ac.","","",550,550,"","","","","","","","","","","","",""]
[null,"Self Prop Harvester/hauling/blow or pack","hr.",4,996.25,"","",670,"","","","","","","","","","","",""]
[null,"Self Propelled harvester only","ac.","","","","","","","","","","","","","","","","",""]
[null,"Self Propelled harvester only","hr.",6,685.83333333333337,"","",529,"","","","","","","","","","","",""]
[]
[null,"Self Prop Harvester with kernel processor only","ac.","","","","","","","","","","","","","","","","",""]
[null,"Self Prop Harvester with kernel processor only","hr.",8,634.375,500,769,477,"","","","","","","","","","","",""]
[null,"Hauling only - trucks","ac.","","","","","","","","","","","","","","","","",""]
[null,"Hauling only - trucks","hr.",4,141.25,"","","","","","","","","","","","","","",""]
[null,"Hauling only - wagons","ac.","","","","","","","","","","","","","","","","",""]
[null,"Hauling only - wagons","hr.",6,134.16666666666666,"","",155.83333333333334,"","","","","","","","",3,138.33333333333334,"",""]
[null,"Packing only","hr.",6,163.33333333333334,"","",155,"","","","",3,180,"","","","","",""]
[null,"Blowing only","hr.",3,81.666666666666671,"","",75,"","","","","","","","","","","",""]
[null,"MANURE HANDLING"]
[null,"SOLID "]
[null,"Loader only","hr.",12,113.33333333333333,75,158.75,113.07692307692308,"","","","",7,118.57142857142857,"","","","","",""]
[null,"Spreader only","hr.",13,135.57692307692307,62,221,138.88888888888889,"","",4,173.75,5,142,"","","","","",""]
[null,"Loader and Spreader","hr.",10,237.5,157.25,303.99999999999989,220,"","","","",6,239.16666666666666,"","","","","",""]
[null,"LIQUID     "]
[null,"Drag hose boom applicator per 1000 imp gal",null,12,13.329166666666666,10.65,16.5,12.744545454545456,"","","","",5,14.6,"","",3,12.833333333333334,"",""]
[null,"Drag hose injection             per 1000 gal",null,"","",20,20,"","","","","","","","","","","","",""]
[null,"Tanker - surface applied only per 1000 imp gal",null,5,11.8,"","",12.25,"","","","","","","","","","","",""]
[null,"Tanker - surface applied only per hour",null,11,311.36363636363637,237.5,400,243.125,"","","","",7,329.28571428571428,"","","","","",""]
[null,"Tanker - surface applied - with incorporation - per 1000 gal",null,"","","","","","","","","","","","","","","","",""]
[null,"Tanker applied-knife injection per 1000 gal",null,"","","","","","","","","","","","","","","","",""]
[null,"Truck transfer ","hr.",5,213,"","",160,"","","","",3,208.33333333333334,"","","","","",""]
[null,"Sand surcharge per 1000 imp gal",null,7,1.9214285714285713,"","",2.8875000000000002,"","","","",4,2.25,"","","","","",""]
[null,"Pit pump agitation","hr.",9,177.77777777777777,146,196,73.020833333333329,"","","","",6,191.66666666666666,"","","","","",""]
[null,null,"day",4,300,"","",null,"","","","","","","","","","","",""]
[null,"Manure boat","hr.",5,401,"","",357,"","","","",3,418.33333333333331,"","","","","",""]
[null,"MISCELLANEOUS"]
[null,"Snow Removal - blade","hr.",12,190,141.25,277.25,142.18181818181819,"","","","",9,206.66666666666666,"","","","","",""]
[null,"Snow blowing","hr.",16,156.5625,90,231.25,139.57142857142858,3,125,"","",8,190.625,"","","","","",""]
[null,"Survey of Short-term Rental Rates charged in 2024"]
[null,"CUSTOM OPERATION",null,"Provincial",null,null,null,null,"Area 1 ",null,"Area  2",null,"Area  3",null,"Area  4",null,"Area  5",null,"Area  6"]
[null,null,"Unit","# ",2024,"2024 Percentile",null,2021,"# ",2024,"# ",2024,"# ",2024,null,2024,null,2024,null,2024]
[null,null,null,null,"ave.","15th","85th","ave.",null,"ave.",null,"ave.",null,"ave.","# ","ave.","# ","ave.","# ","ave."]
[null,"TRACTOR RENTALS"]
[null,"Tractor ","hr.",10,98.9,51.4,141.24999999999997,116,"","","","",6,83.166666666666671,"","","","","",""]
[null,null,"hp.hr",5,0.41799999999999998,"","",0.39833333333333337,"","","","",3,0.43,"","","","","",""]
[]
[]
[]
[null,"End of worksheet"]